{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M9"]
[]
[]
[]
[]
["","","","","","2AMXM40M4V1B9","2AMXM50M4V1B9"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","552"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","852"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","350"]
["Βάρος","Μονάδα","","","kg","36","41"]
["Κινητήρας ανεμιστήρα","Ταχύτητα","Ψύξη","Κινητήρας ανεμιστήρα-=-Ταχύτητα-=-Ψύξη-=-Εξαιρετικά χαμηλές-=-σ.α.λ.","σ.α.λ.","500"]
["","","Θέρμανση","Κινητήρας ανεμιστήρα-=-Ταχύτητα-=-Θέρμανση-=-Εξαιρετικά χαμηλές-=-σ.α.λ.","σ.α.λ.","320"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","-10","-10"]
["","","","Μέγ.","°CDB","46","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-15","-15"]
["","","","Μέγ.","°CWB","18","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","46","48"]
["","Θέρμανση","","Υψ.","dBA","48","50"]
["Ψυκτικό μέσο","Τύπος","","","","R-32","R-32"]
["","Φορτίο","","","kg","0.88","1.15"]
["","Φορτίο","","","tCO2Eq","0.60","0.78"]
["","GWP","","","","675","675"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","20 (1)","20 (1)"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 20 m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 20 m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","15","15"]
["","","ΕΣ.-ΕΣ.","Μέγ.","m","7.5","7.5"]
["","Συνολικό μήκος σωληνώσεων","Σύστημα","Πραγματικό","m","30","30"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["","Screw bag","","","","1","1"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","220-230-240","220-230-240"]
["Σημειώσεις","","","","","(1) - Για ένα δωμάτιο","(1) - Για ένα δωμάτιο"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","","552"]
["","","","Πλάτος","mm","","852"]
["","","","Βάθος","mm","","350"]
["Κινητήρας ανεμιστήρα","Ταχύτητα","Ψύξη","Εξαιρετικά χαμηλές","σ.α.λ.","","500"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","σ.α.λ.","","500"]
["Στάνταρτ εξαρτήματα","Reducer assembly","","","","","1"]