{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":8,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXS-F"]
[]
[]
[]
[]
["","","","","","4MXS68F3V1B2","4MXS68F3V1B","4MXS68F2V1B"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Ονομ.","dBA","49","49"]
["","Ψύξη","","Ονομ.","dBA","48","48"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1","1"]
["","Τάπα εξόδου αποστράγγισης συμπυκνωμάτων","","","","1","1"]
["","Συγκρότημα συστολής","","","","1","1"]
["Ψυκτικό μέσο","Charge","","","TCO2Eq","5.4","5.4"]
["","GWP","","","","2,087.5","2,087.5"]
["","Φορτίο","","","kg","2.6","2.6"]
["","Type","","","","R-410A","R-410A"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Μέγ.","°CDB","46"]
["","","","Ελάχ.","°CDB","-10"]
["","Θέρμανση","Περιβάλλον","Μέγ.","°CWB","18"]
["","","","Ελάχ.","°CWB","-15"]
["Συνδέσεις σωληνώσεων","Υψομετρική διαφορά","ΕΣ.-ΕΣ.","Μέγ.","m","7.5"]
["","","ΕΣ.-ΕΞ.","Μέγ.","m","15"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 30 m)"]
["","Συνολικό μήκος σωληνώσεων","Σύστημα","Πραγματικό","m","60"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","936","936"]
["","","","Βάθος","mm","300","300"]
["","","","Ύψος","mm","735","735"]
["Βάρος","Μονάδα","","","kg","58","58"]
["Power supply","Φάση","","","","1~","1~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","230","230"]
["Σημειώσεις","","","","","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19,0°CWB / εξ. θερμοκρασία 35°CDB, ισοδύναμο μήκος σωληνώσεων: 5m","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19,0°CWB / εξ. θερμοκρασία 35°CDB, ισοδύναμο μήκος σωληνώσεων: 5m"]
["","","","","","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 5m","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 5m"]
["","","","","","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]
["Συνδέσεις σωληνώσεων","Υψομετρική διαφορά","ΕΣ.-ΕΣ.","Μέγ.","m","","7.5"]
["","","ΕΣ.-ΕΞ.","Μέγ.","m","","15"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 30 m)"]
["","Συνολικό μήκος σωληνώσεων","Σύστημα","Πραγματικό","m","","60"]
["Συμπιεστής","Τύπος","","","","","Ερμητικά κλειστός συμπιεστής swing"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","","","735"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","","","936"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","","","300"]
["Βάρος","Μονάδα","","","kg","","","58"]
["Συμπιεστής","Τύπος","","","","","","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","","","-10"]
["","","","Μέγ.","°CDB","","","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","","","-15"]
["","","","Μέγ.","°CWB","","","15.5"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Ονομ.","dBA","","","48"]
["","Θέρμανση","","Ονομ.","dBA","","","49"]
["Ψυκτικό μέσο","Τύπος","","","","","","R-410A"]
["","Φορτίο","","","kg","","","2.6"]
["","Φορτίο","","","tCO2Eq","","","5.4"]
["","GWP","","","","","","2087.5"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","","","25"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","","","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 30 m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","","","15"]
["","","ΕΣ.-ΕΣ.","Μέγ.","m","","","7.5"]
["","Συνολικό μήκος σωληνώσεων","Σύστημα","Πραγματικό","m","","","60"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["Τροφοδοσία ισχύος","Φάση","","","","","","1~"]
["","Συχνότητα","","","Hz","","","50"]
["","Τάση","","","V","","","230"]