{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":9,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C"]
[]
[]
[]
[]
["","","","","","ABQ71CV1","ABQ100CV1","ABQ125CV1","ABQ140CV1"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","Εγχειρίδιο εγκατάστασης"]
["","Εγχειρίδιο χειρισμού","","","","Εγχειρίδιο χειρισμού"]
["","Βίδα+Ροδέλα","","","","Βίδα+Ροδέλα"]
["","Ασύρματο τηλεχειριστήριο","","","","Ασύρματο τηλεχειριστήριο"]
["","Σχάρα κλειδώματος καλύμματος","","","","Σχάρα κλειδώματος καλύμματος"]
["","Μπαταρία","","","","Μπαταρία"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","9.52"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","15.88"]
["","Συμπυκνωμάτων","","","","19.05"]
["Power input","Ψύξη","","Ονομ.","kW","0.128"]
["","Θέρμανση","","Ονομ.","kW","0.128"]
["Sound power level","Ψύξη","","","dBA","64"]
["","Θέρμανση","","","dBA","64"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","600"]
["","","","Βάθος","mm","1,007"]
["","","","Ύψος","mm","285"]
["Περίβλημα","Υλικό","","","","Γαλβανισμένος χάλυβας"]
["Βάρος","Μονάδα","","","kg","35"]
["Ανεμιστήρας","Εξωτερική στατική πίεση","","Υψηλή","Pa","90"]
["","","","Ονομ.","Pa","77"]
["","","","Χαμηλή","Pa","64"]
["Power supply","Φάση","","","","1~"]
["","Συχνότητα","","","Hz","50"]
["","Όνομα","","","","V1"]
["","Τάση","","","V","220-240"]
["Ισχύς εισόδου","Θέρμανση","","Ονομ.","kW","","0.109"]
["","Ψύξη","","Ονομ.","kW","","0.109"]
["Ανεμιστήρας","Εξωτερική στατική πίεση","","Υψηλή","Pa","","70","150","150"]
["","","","Χαμηλή","Pa","","45","111","92"]
["Περίβλημα","Υλικό","","","","","Γαλβανισμένος χάλυβας"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","","378","378","378"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","","541","1300","1500"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","","1045","541","541"]
["Βάρος","Μονάδα","","","kg","","44","50","56"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","","22.7","40.5","48.7"]
["","","","Ονομ.","m³/min","","20.5","37","44"]
["","","","Χαμηλή","m³/min","","18.3","34.8","37.9"]
["","","Θέρμανση","Υψ.","m³/min","","22.7","40.5","48.7"]
["","","","Ονομ.","m³/min","","20.5","37.4","43.9"]
["","","","Χαμηλή","m³/min","","18.3","34.8","37.9"]
["","Εξωτερική στατική πίεση","","Ονομ.","Pa","","57","128","122"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","","60","72","73"]
["","Θέρμανση","","","dBA","","60","72","73"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","","41","53","55"]
["","","","Ονομ.","dBA","","38"]
["","","","Χαμηλή","dBA","","36","50","50"]
["","Θέρμανση","","Υψ.","dBA","","41","53","55"]
["","","","Ονομ.","dBA","","38"]
["","","","Χαμηλή","dBA","","36","50","50"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","9.52","9.52","9.52"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","15.88","15.9","15.9"]
["","Αποχέτευση","","","","","19.05"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","","Installation manual"]
["","Wireless remote control","","","","","Wireless remote control"]
["","Cover lock grill","","","","","Cover lock grill"]
["","Battery","","","","","Battery"]
["","Screw+Washer","","","","","Screw+Washer"]
["","Operation manual","","","","","Operation manual"]
["Τροφοδοσία ισχύος","Φάση","","","","","1~"]
["","Συχνότητα","","","Hz","","50"]
["","Τάση","","","V","","220-240"]
["Απόδοση ψύξης","Συνολική απόδοση","","Ονομ.","kW","","","12.10","13.00"]
["Απόδοση σε λειτουργία θέρμανσης","Συνολική απόδοση","","Ονομ.","kW","","","13.5","15.5"]
["Περίβλημα","Χρώμα","","","","","","Γαλβανισμένο χαλυβδοέλασμα / Άβαφο","Γαλβανισμένο χαλυβδοέλασμα / Άβαφο"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Μέτρια","m³/min","","","37","44"]
["","","Θέρμανση","Μέτρια","m³/min","","","37.4","43.9"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Μέτρια","dBA","","","52","53"]
["","Θέρμανση","","Μέτρια","dBA","","","52","53"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","","","ARCWLA","ARCWLA"]