{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":10,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C"]
[]
[]
[]
[]
["","","","","ADEQ35C2VEB","ADEQ50C2VEB","ADEQ60C2VEB","ADEQ71C2VEB","ADEQ100C2VEB","ADEQ125C2VEB"]
["Στάθμη ηχ. πίεσης","Θέρμανση","Υψ.","dBA","37","37","31","31","36","38"]
["","","Ονομ.","dBA","37","37","31","31","36","38"]
["","","Μέτρια","dBA","34","34","28","28","33","35"]
["","","Χαμηλή","dBA","29","29","25","25","30","32"]
["","Ψύξη","Μέτρια","dBA","32","32","28","28","32","35"]
["","","Χαμηλή","dBA","29","29","25","25","30","32"]
["","","Υψ.","dBA","35","35","30","30","34","37"]
["","","Ονομ.","dBA","35","35","30","30","34","37"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο χειρισμού","","","1","1","1","1","1","1"]
["","Εγχειρίδιο εγκατάστασης","","","1","1","1","1","1","1"]
["","Εύκαμπτος σωλήνας αποστράγγισης συμπυκνωμάτων","","","1","1","1","1","1","1"]
["","Μεταλλικός σφιγκτήρας εύκαμπτου σωλήνα αποστράγγισης συμπυκνωμάτων","","","1","1","1","1","1","1"]
["","Ροδέλα για στήριγμα ανάρτησης","","","8","8","8","8","8","8"]
["","Κοχλίες","","","40","40","40","40","40","40"]
["","Μόνωση συνδέσμου","","","2","2","2","2","2","2"]
["","Στεγανοποιητικό παρέμβυσμα","","","5","5","5","5","5","5"]
["","Σφιγκτήρες","","","4","4","4","4","4","4"]
["Ψυκτικό μέσο","GWP","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["Απόδοση ψύξης","Συνολική απόδοση","Ονομ.","kW","","","","","","12.10"]
["Συνδέσεις σωληνώσεων","Υγρού","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35","6.35","9.52","9.52","9.52"]
["","Αερίου","ΕΞ.ΔΙΑΜ.","mm","9.52","12.7","12.7","15.9","15.9","15.9"]
["","Συμπυκνωμάτων","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","dBA","60","60","56","56","58","62"]
["Διαστάσεις","Μονάδα","Πλάτος","mm","700","700","1,000","1,000","1,400","1,400"]
["","","Βάθος","mm","800","800","800","800","800","800"]
["","","Ύψος","mm","245","245","245","245","245","245"]
["Casing","Υλικό","","","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα"]
["","Colour","","","Άβαφο","Άβαφο","Άβαφο","Άβαφο","Άβαφο","Άβαφο"]
["Βάρος","Μονάδα","","kg","28.0","28.0","35.0","35","46","46"]
["Ανεμιστήρας","Εξωτερική στατική πίεση","Υψηλή","Pa","150","150","150","150","150","150"]
["","","Ονομ.","Pa","30","30","30","30","40","50"]
["Απόδοση θέρμανσης","Συνολική απόδοση","Ονομ.","kW","","","","","","13.5"]
["Power supply","Φάση","","","1~","1~","1~","1~","1~","1~"]
["","Συχνότητα","","Hz","50","50","50","50","50","50"]
["","Τάση","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Σημειώσεις","","","","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή."]