{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":11,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXC-B"]
[]
[]
[]
[]
["","","","","","ARXC20BV1B","ARXC25BV1B","ARXC35BV1B","ARXC50BV1B","ARXC60BV1B","ARXC71BV1B"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","45","","","51","54"]
["Ψυκτικό μέσο","Charge","","","TCO2Eq","0.371","","","0.675","0.743"]
["","GWP","","","","675","","","675","675"]
["","Charge","","","kg","0.55","","","1","1.1"]
["","Τύπος","","","","R-32","","","R-32","R-32"]
["Συνδέσεις σωληνώσεων","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","15","","","20","20"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,017 (για μήκος σωληνώσεων μεγαλύτερο από 7,5m)","","","0,017 (για μήκος σωληνώσεων μεγαλύτερο από 7,5m)","0,017 (για μήκος σωληνώσεων μεγαλύτερο από 7,5m)"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing.","","","Ερμητικά κλειστός συμπιεστής swing.","Ερμητικά κλειστός συμπιεστής swing."]
["Διαστάσεις","Μονάδα","","Πλάτος","χιλ.","658","","","845","845"]
["","","","Βάθος","χιλ.","273","","","300","300"]
["","","","Ύψος","χιλ.","550","","","615","615"]
["Βάρος","Μονάδα","","","kg","24","","","39","39"]
["Power supply","Phase","","","","1~","","","1~","1~"]
["","Συχνότητα","","","Hz","50","","","50","50"]
["","Τάση","","","V","220-240","","","220-240","220-240"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","χιλ.","","550","550","","","695"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","χιλ.","","658","658","","","930"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","χιλ.","","273","273","","","350"]
["Βάρος","Μονάδα","","","kg","","24","26","","","45"]
["Συμπιεστής","Τύπος","","","","","Ερμητικά κλειστός συμπιεστής swing.","Ερμητικά κλειστός συμπιεστής swing.","","","Ερμητικά κλειστός συμπιεστής swing."]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","","10","10","","","-10"]
["","","","Μέγ.","°CDB","","46","46","","","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","","-15","-15","","","-15"]
["","","","Μέγ.","°CWB","","18","18","","","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","","45","46","","","54"]
["Ψυκτικό μέσο","Τύπος","","","","","R-32","R-32","","","R-32"]
["","Φορτίο","","","kg","","0.55","0.75","","","1.15"]
["","Φορτίο","","","tCO2Eq","","0.371","0.506","","","0.776"]
["","GWP","","","","","675","675","","","675"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","","20","20","","","30"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","","0,017 (για μήκος σωληνώσεων μεγαλύτερο από 7,5m)","0,017 (για μήκος σωληνώσεων μεγαλύτερο από 7,5m)","","","0,017 (για μήκος σωληνώσεων μεγαλύτερο από 7,5m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","","15","15","","","20"]
["Τροφοδοσία ισχύος","Φάση","","","","","1~","1~","","","1~"]
["","Συχνότητα","","","Hz","","50","50","","","50"]
["","Τάση","","","V","","220-240","220-240","","","220-240"]