{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":11,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXC-D"]
[]
[]
[]
[]
["","","","","","ARXC20DV1B","ARXC25DV1B","ARXC35DV1B","ARXC50DV1B","ARXC60DV1B","ARXC71DV1B"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","","45","46","51","54","54"]
["Ψυκτικό μέσο","GWP","","","","","675.0","675.0","675.0","675.0","675.0"]
["","Φορτίο","","","kg","","0.550","0.750","1.00","1.10","1.15"]
["","Τύπος","","","","","R-32","R-32","R-32","R-32","R-32"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Μέγ.","°CDB","","46","46","46","46","46"]
["","","","Ελάχ.","°CDB","","10","10","-10","-10","-10"]
["","Θέρμανση","Περιβάλλοντος","Μέγ.","°CWB","","18","18","18","18","18"]
["","","","Ελάχ.","°CWB","","-15","-15","-15","-15","-15"]
["Συνδέσεις σωληνώσεων","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","","15.0","15.0","20.0","20.0","20.0"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","","0,017 (για μήκος σωληνώσεων μεγαλύτερο από 7,5m)","0,017 (για μήκος σωληνώσεων μεγαλύτερο από 7,5m)","0,017 (για μήκος σωληνώσεων μεγαλύτερο από 7,5m)","0,017 (για μήκος σωληνώσεων μεγαλύτερο από 7,5m)","0,017 (για μήκος σωληνώσεων μεγαλύτερο από 7,5m)"]
["Sound power level","Ψύξη","","","dBA","","58","60","65","66","69"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","","658","658","845","845","930"]
["","","","Βάθος","mm","","273","273","300","300","350"]
["","","","Ύψος","mm","","550","550","615","615","695"]
["Συμπιεστής","Τύπος","","","","","Ερμητικά κλειστός συμπιεστής swing.","Ερμητικά κλειστός συμπιεστής swing.","Ερμητικά κλειστός συμπιεστής swing.","Ερμητικά κλειστός συμπιεστής swing.","Ερμητικά κλειστός συμπιεστής swing."]
["Βάρος","Μονάδα","","","kg","","24.0","26.0","39.0","39.0","45.0"]
["Power supply","Φάση","","","","","1~","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","","50","50","50","50","50"]
["","Τάση","","","V","","220-240","220-240","220-240","220-240","220-240"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","58"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","550"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","658"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","273"]
["Βάρος","Μονάδα","","","kg","24"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing."]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","10"]
["","","","Μέγ.","°CDB","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-15"]
["","","","Μέγ.","°CWB","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","45"]
["Ψυκτικό μέσο","Τύπος","","","","R-32"]
["","Φορτίο","","","kg","0.55"]
["","Φορτίο","","","tCO2Eq","0.371"]
["","GWP","","","","675.0"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","20"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,017 (για μήκος σωληνώσεων μεγαλύτερο από 7,5m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","15.0"]
["Τροφοδοσία ισχύος","Φάση","","","","1~"]
["","Συχνότητα","","","Hz","50"]
["","Τάση","","","V","220-240"]