{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":10,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-A"]
[]
[]
[]
[]
["","","","","","ARXM25A5V1B","ARXM35A5V1B","ARXM50A5V1B","ARXM60A5V1B","ARXM71A5V1B"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","610","610","734","734","734"]
["","","","Πλάτος","mm","923","923","954","954","954"]
["","","","Βάθος","mm","367","367","401","401","401"]
["Βάρος","Μονάδα","","","kg","36","36","49","49","49"]
["Κινητήρας ανεμιστήρα","Ταχύτητα","Ψύξη","Εξαιρετικά χαμηλές","σ.α.λ.","600","600","500"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","-10","-10","-10","-10","-10"]
["","","","Μέγ.","°CDB","50","50","50 (1), 46 (1)","46","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-21","-21","-21 (1), -15 (1)","-15","-15"]
["","","","Μέγ.","°CWB","18","18","18","18","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Ονομ.","dBA","46","47","48","48","52"]
["","Θέρμανση","","Ονομ.","dBA","47","49","49","49","52"]
["Ψυκτικό μέσο","Τύπος","","","","R-32","R-32","R-32","R-32","R-32"]
["","Φορτίο","","","kg","0.95","0.95","1.1","1.15","1.15"]
["","Φορτίο","","","tCO2Eq","0.65","0.65","0.75","0.78","0.78"]
["","GWP","","","","675","675","675","675","675"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","20","20","30","30","30"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","002 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","002 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","002 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","002 (για μήκος σωληνώσεων μεγαλύτερο από 10m)","0035 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","15","15","20","20","20"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Drain cap","","","","3","3","1","3","3"]
["Εύρος ενεργειακής αποδοτικότητας","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240","220-240","220-240"]
["Σημειώσεις","","","","","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["","","","","","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]
["Στάνταρτ εξαρτήματα","ARXM50A5V1B","","","","","","1"]
["","Drain plug","","","","","","","1","1"]