{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-A8"]
[]
[]
[]
[]
["","","","","","ARXM50A5V1B8"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","610"]
["","","","Πλάτος","mm","923"]
["","","","Βάθος","mm","367"]
["Βάρος","Μονάδα","","","kg","40"]
["Κινητήρας ανεμιστήρα","Ταχύτητα","Ψύξη","Εξαιρετικά χαμηλές","σ.α.λ.","600"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","-10"]
["","","","Μέγ.","°CDB","50 (1), 46 (1)"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-21 (1), -15 (1)"]
["","","","Μέγ.","°CWB","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Ονομ.","dBA","48"]
["","Θέρμανση","","Ονομ.","dBA","49"]
["Ψυκτικό μέσο","Τύπος","","","","R-32"]
["","Φορτίο","","","kg","0.95"]
["","Φορτίο","","","tCO2Eq","0.65"]
["","GWP","","","","675"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","30"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","20"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1"]
["","Drain joint","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","LOT10 Energy Label","","","","1"]
["","Drain cap","","","","3"]
["Τροφοδοσία ισχύος","Φάση","","","","1~"]
["","Συχνότητα","","","Hz","50"]
["","Τάση","","","V","220-240"]
["Σημειώσεις","","","","","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["","","","","","(3) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]