{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXN-M6"]
[]
[]
[]
[]
["","","","","","ARXN20MV16","ARXN25MV16","ARXN35MV16","ARXN50MV16","ARXN60MV16"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","550","550","550","753","753"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","658","658","658","855","855"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","289","289","289","328","328"]
["Βάρος","Μονάδα","","","kg","29","29","31","44","44"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","10","10","10","-10","-10"]
["","","","Μέγ.","°CDB","46","46","46","46","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-15","-15","-15","-15","-15"]
["","","","Μέγ.","°CWB","18","18","18","18","18"]
["Ψυκτικό μέσο","Τύπος","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Φορτίο","","","kg","0.74","0.74","1.00","1.45","1.45"]
["","Φορτίο","","","tCO2Eq","1.5","1.5","2.1","3.0","3.0"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","20","20","20","30","30"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240","220-240","220-240"]