{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":13,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXN-NB9"]
[]
[]
[]
[]
["","","","","","ARXN25NV1B9","ARXN25N5V1B9","ARXN25N6V1B9","ARXN35N6V1B9","ARXN50NV1B9","ARXN60NV1B9","ARXN35N5V1B9 (Archived)","ARXN35NV1B9 (Archived)"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","","","","46","51","51","46","46"]
["Στάνταρτ εξαρτήματα","Σύνδεσμος εξόδου συμπυκνωμάτων","","","","","","","Σύνδεσμος εξόδου συμπυκνωμάτων","Σύνδεσμος εξόδου συμπυκνωμάτων","Σύνδεσμος εξόδου συμπυκνωμάτων","Σύνδεσμος εξόδου συμπυκνωμάτων","Σύνδεσμος εξόδου συμπυκνωμάτων"]
["","Τάπα εξόδου αποστράγγισης συμπυκνωμάτων","","","","","","","Τάπα εξόδου αποστράγγισης συμπυκνωμάτων","Τάπα εξόδου αποστράγγισης συμπυκνωμάτων","Τάπα εξόδου αποστράγγισης συμπυκνωμάτων","Τάπα εξόδου αποστράγγισης συμπυκνωμάτων","Τάπα εξόδου αποστράγγισης συμπυκνωμάτων"]
["Ψυκτικό μέσο","Charge","","","TCO2Eq","","","","2.1","3.0","3.0","2.1","2.1"]
["","GWP","","","","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Φορτίο","","","kg","","","","1.00","1.45","1.45","1.00","1.00"]
["","Τύπος","","","","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Piping connections","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","","","","10.0","10.0","10.0","10.0","10.0"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","","","","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 7.5 m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 7.5 m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 7.5 m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 7.5 m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 7.5 m)"]
["Συμπιεστής","Type","","","","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","","","","658","855","855","658","658"]
["","","","Βάθος","mm","","","","289","328","328","289","289"]
["","","","Ύψος","mm","","","","550","628","753","550","550"]
["Βάρος","Μονάδα","","","kg","","","","26","37","44","26","26"]
["Power supply","Φάση","","","","","","","1~","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","","","","50","50","50","50","50"]
["","Τάση","","","V","","","","220-240","220-240","220-240","220-240","220-240"]
["Σημειώσεις","","","","","","","","(1) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(1) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(1) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(1) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(1) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]
["","","","","","","","","(2) - Όλες οι μονάδες ελέγχονται και συμμορφώνονται με το ISO5151 (μονάδα χωρίς αεραγωγό) ή ISO13253 (μονάδα με αεραγωγό)","(2) - Όλες οι μονάδες ελέγχονται και συμμορφώνονται με το ISO5151 (μονάδα χωρίς αεραγωγό) ή ISO13253 (μονάδα με αεραγωγό)","(2) - Όλες οι μονάδες ελέγχονται και συμμορφώνονται με το ISO5151 (μονάδα χωρίς αεραγωγό) ή ISO13253 (μονάδα με αεραγωγό)","(2) - Όλες οι μονάδες ελέγχονται και συμμορφώνονται με το ISO5151 (μονάδα χωρίς αεραγωγό) ή ISO13253 (μονάδα με αεραγωγό)","(2) - Όλες οι μονάδες ελέγχονται και συμμορφώνονται με το ISO5151 (μονάδα χωρίς αεραγωγό) ή ISO13253 (μονάδα με αεραγωγό)"]
["","","","","","","","","(3) - Όλες οι προδιαγραφές μπορεί να τροποποιηθούν από τον κατασκευαστή χωρίς προηγούμενη ειδοποίηση.","(3) - Όλες οι προδιαγραφές μπορεί να τροποποιηθούν από τον κατασκευαστή χωρίς προηγούμενη ειδοποίηση.","(3) - Όλες οι προδιαγραφές μπορεί να τροποποιηθούν από τον κατασκευαστή χωρίς προηγούμενη ειδοποίηση.","(3) - Όλες οι προδιαγραφές μπορεί να τροποποιηθούν από τον κατασκευαστή χωρίς προηγούμενη ειδοποίηση.","(3) - Όλες οι προδιαγραφές μπορεί να τροποποιηθούν από τον κατασκευαστή χωρίς προηγούμενη ειδοποίηση."]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","550","550","550"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","658","658","658"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","289","289","289"]
["Βάρος","Μονάδα","","","kg","24","24","24"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","10","10","10"]
["","","","Μέγ.","°CDB","46","46","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-15","-15","-15"]
["","","","Μέγ.","°CWB","18","18","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","45","45","45"]
["Ψυκτικό μέσο","Τύπος","","","","R-410A","R-410A","R-410A"]
["","Φορτίο","","","kg","0.74","0.74","0.74"]
["","Φορτίο","","","tCO2Eq","1.5","1.5","1.5"]
["","GWP","","","","2087.5","2087.5","2087.5"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","20","20","20"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 7.5 m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 7.5 m)","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 7.5 m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","10.0","10.0","10.0"]
["Στάνταρτ εξαρτήματα","Drain joint","","","","Drain joint","Drain joint","Drain joint"]
["","Drain plug","","","","Drain plug","Drain plug","Drain plug"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240"]