{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS25L3V1B","ARXS35L3V1B"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","","48"]
["","","","Χαμηλή","dBA","","45"]
["Στάνταρτ εξαρτήματα","1","","","","","550"]
["Ψυκτικό μέσο","Charge","","","kg","","2.5"]
["","Type","","","","","1.2"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Εξαιρετικά χαμηλές","m³/min","","30.1"]
["","","","Εξαιρετικά χαμηλές","cfm","","1,063"]
["Κινητήρας ανεμιστήρα","Ταχύτητα","Ψύξη","Εξαιρετικά χαμηλές","rpm","","740"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","rpm","","-15"]
["Εύρος λειτουργίας","Θέρμανση","Περιβάλλον","Ελάχ.","°CWB","","20"]
["","","","Μέγ.","°CWB","","10"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Χαμηλή","dBA","","44"]
["","","","Υψ.","dBA","","48"]
["Συμπιεστής","Τύπος","","","","","Ερμητικά κλειστός συμπιεστής swing"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","","285"]
["","","","Βάθος","mm","","612"]
["","","","Ύψος","mm","","765"]
["Βάρος","Μονάδα","","","kg","","34"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Εξαιρετικά χαμηλές","cfm","","904"]
["","","","Εξαιρετικά χαμηλές","m³/min","","25.6"]
["Power supply","Φάση","","","","","1~"]
["","Συχνότητα","","","Hz","","50"]
["","Τάση","","","V","","220-240"]
["Σημειώσεις","","","","","(1) - 220V","(1) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]
["","","","","","(2) - 230V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 230V"]
["","","","","","","(4) - 240V"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Εξαιρετικά χαμηλές","m³/min","30.1"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","m³/min","25.6"]
["","","","Εξαιρετικά χαμηλές","cfm","1063"]
["","","Θέρμανση","Εξαιρετικά χαμηλές","cfm","904"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","550"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","765"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","285"]
["Βάρος","Μονάδα","","","kg","34"]
["Κινητήρας ανεμιστήρα","Ταχύτητα","Ψύξη","Κινητήρας ανεμιστήρα-=-Ταχύτητα-=-Ψύξη-=-Εξαιρετικά χαμηλές-=-σ.α.λ.","rpm","780"]
["","","Θέρμανση","Κινητήρας ανεμιστήρα-=-Ταχύτητα-=-Θέρμανση-=-Εξαιρετικά χαμηλές-=-σ.α.λ.","rpm","740"]
["Συμπιεστής","Τύπος","","","","Ερμητικά κλειστός συμπιεστής swing"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","10"]
["","","","Μέγ.","°CDB","46"]
["","Θέρμανση","Περιβάλλοντος","Ελάχ.","°CWB","-15"]
["","","","Μέγ.","°CWB","18"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","46"]
["","Θέρμανση","","Υψ.","dBA","47"]
["","","","Χαμηλή","dBA","44"]
["Ψυκτικό μέσο","Τύπος","","","","R-410A"]
["","Φορτίο","","","kg","1.0"]
["","Φορτίο","","","tCO2Eq","2.1"]
["","GWP","","","","2087.5"]
["Συνδέσεις σωληνώσεων","Μήκος σωληνώσεων","Μέγ.","OU - IU","m","20"]
["","Πρόσθετο φορτίο ψυκτικού","","","kg/m","0,02 (για μήκος σωληνώσεων μεγαλύτερο από 10m)"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","15"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain plug","","","","1"]
["Τροφοδοσία ισχύος","Φάση","","","","1~"]
["","Συχνότητα","","","Hz","50"]
["","Τάση","","","V","220-240"]