{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-J3"]
[]
[]
[]
[]
["","","","","","ATX20J3V1B","ATX25J3V1B","ATX35J3V1B"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.03","0.03","0.030"]
["","Θέρμανση","","Ονομ.","kW","0.04","0.04","0.040"]
["Περίβλημα","Χρώμα","","","","Λευκό","Λευκό","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","198","198","198"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","770","770","770"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","283","283","283"]
["Βάρος","Μονάδα","","","kg","7","7","7.00"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","9.1","9.2","9.3"]
["","","","Μέτρια","m³/min","7.4","7.6","7.7"]
["","","","Χαμηλή","m³/min","5.9","6","6.1"]
["","","","Αθόρυβη λειτουργία","m³/min","4.7","4.8","4.9"]
["","","Θέρμανση","Υψ.","m³/min","9.4","9.7","10.1"]
["","","","Μέτρια","m³/min","7.8","8","8.4"]
["","","","Χαμηλή","m³/min","6.3","6.3","6.7"]
["","","","Αθόρυβη λειτουργία","m³/min","5.5","5.5","5.7"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","55","55","58"]
["","Θέρμανση","","","dBA","55","55","58"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","39","40","41"]
["","","","Μέτρια","dBA","33","33","34"]
["","","","Χαμηλή","dBA","25","26","27"]
["","","","Αθόρυβη λειτουργία","dBA","22","22","23"]
["","Θέρμανση","","Υψ.","dBA","39","40","41"]
["","","","Μέτρια","dBA","34","34","35"]
["","","","Χαμηλή","dBA","28","28","29"]
["","","","Αθόρυβη λειτουργία","dBA","25","25","26"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","6.35","6.35","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","9.5","9.5","9.50"]
["","Αποχέτευση","","","","18","18","18"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","ARC433A89","ARC433A89","ARC433A89"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Τροφοδοσία ισχύος","Όνομα","","","","V1","V1","V1"]
["","Φάση","","","","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240"]