{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":11,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-KV"]
[]
[]
[]
[]
["","","","","","ATX20K2V1B","ATX20K5V1B","ATX25K2V1B","ATX25K5V1B","ATX35K5V1B","ATX35K2V1B (Archived)"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","","","","","","43"]
["","","","Μέτρια","dBA","","","","","","35"]
["","","","Αθόρυβη λειτουργία","dBA","","","","","","26"]
["","","","Χαμηλή","dBA","","","","","","29"]
["","Ψύξη","","Μέτρια","dBA","","","","","","34"]
["","","","Αθόρυβη λειτουργία","dBA","","","","","","20"]
["","","","Χαμηλή","dBA","","","","","","27"]
["","","","Υψ.","dBA","","","","","","43"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","","","","","","1"]
["","Εγχειρίδιο χειρισμού","","","","","","","","","1"]
["","Τηλεχειριστήριο υπερύθρων","","","","","","","","","1"]
["","Μπαταρίες ξηρού στοιχείου ΑΑ","","","","","","","","","2"]
["","Υποδοχή τηλεχειριστηρίου","","","","","","","","","1"]
["","Πλάκα στήριξης","","","","","","","","","1"]
["","Φωτοκαταλυτικό φίλτρο αέρα από τιτάνιο με επικάλυψη απατίτη.","","","","","","","","","2"]
["","Βίδες στερέωσης εσωτερικής μονάδας","","","","","","","","","2"]
["Συστήματα ελέγχου","Wired remote control","","","","","","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","","","","","","ARC480A11"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","","","","","","6.35"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","","","","","","9.50"]
["","Συμπυκνωμάτων","","","","","","","","","18"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","","","","","","0.024"]
["","Θέρμανση","","Ονομ.","kW","","","","","","0.029"]
["Sound power level","Ψύξη","","","dBA","","","","","","58"]
["","Θέρμανση","","","dBA","","","","","","58"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","","","","","","770"]
["","","","Βάθος","mm","","","","","","225"]
["","","","Ύψος","mm","","","","","","286"]
["Περίβλημα","Χρώμα","","","","","","","","","Λευκό"]
["Βάρος","Μονάδα","","","kg","","","","","","9.0"]
["Power supply","Φάση","","","","","","","","","1~"]
["","Συχνότητα","","","Hz","","","","","","50"]
["","Όνομα","","","","","","","","","V1"]
["","Τάση","","","V","","","","","","220-240"]
["Σημειώσεις","","","","","","","","","","(1) - SL: Αθόρυβη λειτουργία ανεμιστήρα για τη ρύθμιση ταχύτητας ροής αέρα"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.018","0.018","0.02","0.02","0.024"]
["","Θέρμανση","","Ονομ.","kW","0.022","0.022","0.023","0.023","0.029"]
["Περίβλημα","Χρώμα","","","","Λευκό","Λευκό","Λευκό","Λευκό","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","286","286","286","286","286"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","770","770","770","770","770"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","225","225","225","225","225"]
["Βάρος","Μονάδα","","","kg","8.5","8.5","8.5","8.5","9"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","9.9","9.9","10.4","10.4","11.8"]
["","","","Μέτρια","m³/min","7.8","7.8","8","8","8.2"]
["","","","Χαμηλή","m³/min","5.8","5.8","6.1","6.1","6.3"]
["","","","Αθόρυβη λειτουργία","m³/min","4.8","4.8","4.8","4.8","4.9"]
["","","Θέρμανση","Υψ.","m³/min","10.9","10.9","11.1","11.1","12.8"]
["","","","Μέτρια","m³/min","8.5","8.5","8.5","8.5","8.5"]
["","","","Χαμηλή","m³/min","6.4","6.4","6.7","6.7","6.9"]
["","","","Αθόρυβη λειτουργία","m³/min","5.2","5.2","5.2","5.2","5.2"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","55","55","55","55","58"]
["","Θέρμανση","","","dBA","55","55","55","55","58"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","39","39","40","40","43"]
["","","","Μέτρια","dBA","33","33","33","33","34"]
["","","","Χαμηλή","dBA","25","25","26","26","27"]
["","","","Αθόρυβη λειτουργία","dBA","20","20","20","20","20"]
["","Θέρμανση","","Υψ.","dBA","39","39","40","40","43"]
["","","","Μέτρια","dBA","34","34","34","34","35"]
["","","","Χαμηλή","dBA","28","28","28","28","29"]
["","","","Αθόρυβη λειτουργία","dBA","23","23","23","23","26"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","6.35","6.35","6.35","6.35","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","9.5","9.5","9.5","9.5","9.5"]
["","Αποχέτευση","","","","18","18","18","18","18"]
["Συστήματα ελέγχου","Infrared remote control","","","","ARC480A11","ARC480A11","","","ARC480A11"]
["Χειριστήρια","Τηλεχειριστήριο με καλώδιο","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1","1","1","1","1"]
["","AA dry-cell batteries","","","","2","","2"]
["","Operation manual","","","","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1"]
["Τροφοδοσία ισχύος","Όνομα","","","","V1","V1","V1","V1","V1"]
["","Φάση","","","","1~","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50","50","50"]
["","Τάση","","","V","220-240","220-240","220-240","220-240","220-240"]
["Στάνταρτ εξαρτήματα","AAA dry-cell batteries","","","","","2","","2","2"]
["Χειριστήρια","Τηλεχειριστήριο υπερύθρων","","","","","","ARC480A11","ARC480A11"]
["Στάνταρτ εξαρτήματα","Titanium apatite photocatalytic air purification filter","","","","","","2"]