{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXC-A"]
[]
[]
[]
[]
["","","","","ATXC25AV1B","ATXC35AV1B","ATXC50AV1B","ATXC60AV1B"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","Υψ.","dBA","","41"]
["","","Μέτρια","dBA","","34"]
["","","Αθόρυβη λειτουργία","dBA","","22"]
["","","Χαμηλή","dBA","","30"]
["Ισχύς εισόδου","Θέρμανση","Ονομ.","kW","","1,280"]
["Sound power level","Θέρμανση","","dBA","","54"]
["Διαστάσεις","Μονάδα","Πλάτος","mm","","859"]
["","","Βάθος","mm","","209"]
["","","Ύψος","mm","","288"]
["Περίβλημα","Υλικό","","","","Πολυστυρένιο υψηλής αντοχής"]
["","Χρώμα","","","","Λευκό"]
["Βάρος","Μονάδα","","kg","","9.00"]
["Power supply","Φάση","","","","1~"]
["","Συχνότητα","","Hz","","50"]
["","Τάση","","V","","220-240"]
["Σημειώσεις","","","","","(1) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή."]
["Ισχύς εισόδου","Θέρμανση","Ονομ.","kW","830","","1550","1810"]
["Περίβλημα","Χρώμα","","","Λευκό","","Λευκό","Λευκό"]
["","Υλικό","","","Πολυστυρένιο υψηλής αντοχής","","Πολυστυρένιο υψηλής αντοχής","Πολυστυρένιο υψηλής αντοχής"]
["Διαστάσεις","Μονάδα","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","288","","310","310"]
["","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","859","","1120","1120"]
["","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","209","","237","237"]
["Βάρος","Μονάδα","","kg","9.00","","14.0","14.0"]
["Στάθμη ηχητικής ισχύος","Θέρμανση","","dBA","53","","53","61"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","Υψ.","dBA","40","","40","43"]
["","","Μέτρια","dBA","34","","38","41"]
["","","Χαμηλή","dBA","29","","35","37"]
["","","Αθόρυβη λειτουργία","dBA","21","","32","33"]
["Τροφοδοσία ισχύος","Φάση","","","1~","","1~","1~"]
["","Συχνότητα","","Hz","50","","50","50"]
["","Τάση","","V","220-240","","220-240","220-240"]