{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":10,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXC-B / ARXC-B"]
[]
[]
[]
[]
["","","","","ATXC20BV1B / ARXC20BV1B","ATXC25BV1B / ARXC25BV1B","ATXC35BV1B / ARXC35BV1B","ATXC50BV1B / ARXC50BV1B","ATXC60BV1B / ARXC60BV1B","ATXC71BV1B / ARXC71BV1B"]
["Απόδοση ψύξης","Ελάχ.","","kW","1.30","1.30","1.30","1.37","1.80","2.30"]
["","Μέγ.","","kW","3.00","3.00","4.00","6.20","7.00","7.30"]
["Ονομαστική απόδοση","EER","","","3.33","3.30","3.30","3.25","3.25","2.95"]
["","COP","","","3.73","3.76","3.72","3.71","3.71","3.21"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A","A","A","A","A","C"]
["","","Θέρμανση","","A","A","A","A","A","C"]
["Απόδοση θέρμανσης","Ελάχ.","","kW","1.30","1.30","1.30","1.36","1.48","2.30"]
["","Μέγ.","","kW","4.00","4.00","4.80","6.60","8.00","9.00"]