{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":7,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXD-A"]
[]
[]
[]
[]
["","","","","","ATXD25A5V1B","ATXD35A5V1B"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","","0.032"]
["","Θέρμανση","","Ονομ.","kW","","0.032"]
["Περίβλημα","Χρώμα","","","","","Λευκό"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","","286"]
["","","","Πλάτος","mm","","770"]
["","","","Βάθος","mm","","225"]
["Βάρος","Μονάδα","","","kg","","9.00"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","","11.0"]
["","","","Μέτρια","m³/min","","8.5"]
["","","","Χαμηλή","m³/min","","6.8"]
["","","","Αθόρυβη λειτουργία","m³/min","","5.4"]
["","","Θέρμανση","Υψ.","m³/min","","11.5"]
["","","","Μέτρια","m³/min","","9.4"]
["","","","Χαμηλή","m³/min","","7.7"]
["","","","Αθόρυβη λειτουργία","m³/min","","6.3"]
["Sound power level","Ψύξη","","","dBA","","58"]
["","Θέρμανση","","","dBA","","58"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","","43"]
["","","","Μέτρια","dBA","","34"]
["","","","Χαμηλή","dBA","","27"]
["","","","Αθόρυβη λειτουργία","dBA","","20"]
["","Θέρμανση","","Υψ.","dBA","","40"]
["","","","Μέτρια","dBA","","35"]
["","","","Χαμηλή","dBA","","29"]
["","","","Αθόρυβη λειτουργία","dBA","","21"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","","6"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","","9.50"]
["","Drain","","","","","18"]
["Συστήματα ελέγχου","Infrared remote control","","","","","ARC480A78"]
["","Wired remote control","","","","","BRC944B2, BRC073A1"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","","1"]
["","Εγχειρίδιο χειρισμού","","","","","1"]
["","Τηλεχειριστήριο υπερύθρων","","","","","1"]
["","Μπαταρίες ξηρού στοιχείου ΑΑΑ","","","","","2"]
["","Υποδοχή τηλεχειριστηρίου","","","","","1"]
["","Πλάκα στήριξης","","","","","1"]
["","Αποσμητικό φίλτρο τιτανίου με επικάλυψη απατίτη","","","","","1"]
["","Ασημί φίλτρο σωματιδίων","","","","","1"]
["","Βίδες στερέωσης εσωτερικής μονάδας","","","","","2"]
["","Γενικές Προφυλάξεις Ασφαλείας","","","","","1"]
["Power supply","Φάση","","","","","1~"]
["","Συχνότητα","","","Hz","","50"]
["","Τάση","","","V","","220-240"]
["Σημειώσεις","","","","","","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19°CDB, εξωτερική θερμ. 35°CDB, ισοδύναμο μήκος σωληνώσεων: 5m / υψομετρική διαφορά: 0m"]
["","","","","","","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 5m (οριζόντια)"]
["","","","","","","(3) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["Στάθμη ηχητικής ισχύος","Θέρμανση","","","dBA","55"]
["","Ψύξη","","","dBA","55"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","286"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","770"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","225"]
["Βάρος","Μονάδα","","","kg","8.5"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","40"]
["","","","Χαμηλή","dBA","26"]
["","Θέρμανση","","Υψ.","dBA","40"]
["","","","Χαμηλή","dBA","28"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Infrared remote control","","","","1"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Τροφοδοσία ισχύος","Φάση","","","","1~"]
["","Συχνότητα","","","Hz","50"]
["","Τάση","","","V","220-240"]