{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":95,"n_cols":13,"rows_kept":95,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R"]
[]
[]
[]
[]
["","","","","","ATXM20R2V1B §$ ATXM20R5V1B","ATXM20R2V1B","ATXM20R5V1B","ATXM25R2V1B","ATXM25R5V1B","ATXM35R2V1B","ATXM35R5V1B","ATXM50R2V1B"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Υψ.","dBA","39"]
["","","","Μέτρια","dBA","34"]
["","","","Αθόρυβη λειτουργία","dBA","20"]
["","","","Χαμηλή","dBA","26"]
["","Ψύξη","","Μέτρια","dBA","33"]
["","","","Αθόρυβη λειτουργία","dBA","19"]
["","","","Χαμηλή","dBA","25"]
["","","","Υψ.","dBA","41"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1"]
["","Εγχειρίδιο χειρισμού","","","","1"]
["","Ασύρματο τηλεχειριστήριο","","","","1"]
["","Μπαταρίες ξηρού στοιχείου ΑΑΑ","","","","2"]
["","Υποδοχή τηλεχειριστηρίου","","","","1"]
["","Πλάκα στήριξης","","","","1"]
["","Αποσμητικό φίλτρο τιτανίου με επικάλυψη απατίτη","","","","1"]
["","Βίδες στερέωσης εσωτερικής μονάδας","","","","2"]
["","Κιτ αντάπτορα WLAN","","","","1"]
["Συστήματα ελέγχου","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A67"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","6.35"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","9.50"]
["","Συμπυκνωμάτων","","","","18"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.029"]
["","Θέρμανση","","Ονομ.","kW","0.023"]
["Sound power level","Ψύξη","","","dBA","58"]
["","Θέρμανση","","","dBA","55"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","778"]
["","","","Βάθος","mm","272"]
["","","","Ύψος","mm","295"]
["Περίβλημα","Χρώμα","","","","Λευκό"]
["Βάρος","Μονάδα","","","kg","10.0"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Υψ.","m³/min","9.3"]
["","","","Μέτρια","m³/min","8.2"]
["","","","Χαμηλή","m³/min","6.2"]
["","","","Αθόρυβη λειτουργία","m³/min","5.1"]
["","","Ψύξη","Χαμηλή","m³/min","5.7"]
["","","","Μέτρια","m³/min","7.5"]
["","","","Υψ.","m³/min","10.5"]
["","","","Αθόρυβη λειτουργία","m³/min","4.3"]
["Power supply","Φάση","","","","1~"]
["","Όνομα","","","","V1"]
["","Συχνότητα","","","Hz","50"]
["","Τάση","","","V","220-240"]
["Σημειώσεις","","","","","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19,0°CWB / εξ. θερμοκρασία 35°CDB, 24°CWB, ισοδύναμο μήκος σωληνώσεων: 5m"]
["","","","","","(2) - Θέρμανση: εσωτερική θερμοκρ. 20°CDB, εξωτερική θερμ. 7°CDB, 6°CWB,  ισοδύναμες σωληνώσεις ψυκτικού: 5m"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","","0.029","0.029","0.029","0.029","0.03","0.03","0.03"]
["","Θέρμανση","","Ονομ.","kW","","0.023","0.023","0.022","0.022","0.027","0.027","0.032"]
["Περίβλημα","Χρώμα","","","","","Λευκό","Λευκό","Λευκό","Λευκό","Λευκό","Λευκό","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","","295","295","295","295","295","295","299"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","","778","778","778","778","778","778","998"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","","272","272","272","272","272","272","292"]
["Βάρος","Μονάδα","","","kg","","10","10","10","10","10","10","14.5"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","","10.5","10.5","10.5","10.5","11.3","11.3","15.8"]
["","","","Μέτρια","m³/min","","7.5","7.5","7.6","7.6","7.8","7.8","14"]
["","","","Χαμηλή","m³/min","","5.7","5.7","5.7","5.7","6","6","11.4"]
["","","","Αθόρυβη λειτουργία","m³/min","","4.3","4.3","4.1","4.1","4.2","4.2","8.3"]
["","","Θέρμανση","Υψ.","m³/min","","9.3","9.3","9.8","9.8","9.8","9.8","15.8"]
["","","","Μέτρια","m³/min","","8.2","8.2","8","8","8.5","8.5","14.2"]
["","","","Χαμηλή","m³/min","","6.2","6.2","6.3","6.3","6.5","6.5","12"]
["","","","Αθόρυβη λειτουργία","m³/min","","5.1","5.1","4.9","4.9","4.9","4.9","10.5"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","","58","58","58","58","58","58","58"]
["","Θέρμανση","","","dBA","","55","55","55","55","55","55","58"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","","41","41","41","41","45","45","44"]
["","","","Μέτρια","dBA","","33","33","33","33","33","33","40"]
["","","","Χαμηλή","dBA","","25","25","25","25","25","25","36"]
["","","","Αθόρυβη λειτουργία","dBA","","19","19","19","19","19","19","27"]
["","Θέρμανση","","Υψ.","dBA","","39","39","39","39","39","39","43"]
["","","","Μέτρια","dBA","","34","34","34","34","35","35","39"]
["","","","Χαμηλή","dBA","","26","26","27","27","28","28","34"]
["","","","Αθόρυβη λειτουργία","dBA","","20","20","20","20","20","20","31"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","9.5","9.5","9.5","9.5","9.5","9.5","12.7"]
["","Αποχέτευση","","","","","18","18","18","18","18","18","18"]
["Συστήματα ελέγχου","Infrared remote control","","","","","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67"]
["Χειριστήρια","Τηλεχειριστήριο με καλώδιο","","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","","2","2","2","2","2","2","2"]
["","WLAN adapter kit","","","","","1","1","1","1","1","1","1"]
["","Operation manual","","","","","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","1","1","1","1","1","1","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","1","1"]
["Τροφοδοσία ισχύος","Όνομα","","","","","V1","V1","V1","V1","V1","V1","V1"]
["","Φάση","","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Συχνότητα","","","Hz","","50","50","50","50","50","50","50"]
["","Τάση","","","V","","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Στάνταρτ εξαρτήματα","Silver particle filter","","","","","","","","","","","1"]