{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":70,"n_cols":9,"rows_kept":70,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXN-NB9"]
[]
[]
[]
[]
["","","","","","ATXN25NV1B9","ATXN35NV1B9","ATXN50NV1B9","ATXN60NV1B9"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Αθόρυβη λειτουργία","dBA","21","22","","33"]
["","","","Υπερ-υψηλό","dBA","41","42","","46"]
["","","","Χαμηλή","dBA","29","30","","37"]
["","","","Υψ.","dBA","40","41","","43"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1","1","","1"]
["","Εγχειρίδιο χειρισμού","","","","1","1","","1"]
["","Ασύρματο τηλεχειριστήριο","","","","1","1","","1"]
["","Μπαταρίες","","","","Μπαταρίες","Μπαταρίες","","Μπαταρίες"]
["","Υποδοχή τηλεχειριστηρίου","","","","1","1","","1"]
["","Πλάκα στήριξης","","","","1","1","","1"]
["","Φίλτρο από τιτάνιο με επικάλυψη απατίτη","","","","Φίλτρο από τιτάνιο με επικάλυψη απατίτη","Φίλτρο από τιτάνιο με επικάλυψη απατίτη","","Φίλτρο από τιτάνιο με επικάλυψη απατίτη"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35","","6.35"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","9.50","9.50","","15.90"]
["","Συμπυκνωμάτων","","","","16.5","16.5","","16.5"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","693.00","1,060.00","","1,931.00"]
["","Θέρμανση","","Ονομ.","kW","700.00","950.00","","1,680.00"]
["Sound power level","Ψύξη","","","dBA","53","54","","61"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","859","859","","1,124"]
["","","","Βάθος","mm","209","209","","237"]
["","","","Ύψος","mm","288","288","","310"]
["Περίβλημα","Υλικό","","","","Πολυστυρένιο υψηλής αντοχής","Πολυστυρένιο υψηλής αντοχής","","Πολυστυρένιο υψηλής αντοχής"]
["","Χρώμα","","","","Λευκό","Λευκό","","Λευκό"]
["Βάρος","Μονάδα","","","kg","9.0","9.0","","14.0"]
["Power supply","Φάση","","","","1~","1~","","1~"]
["","Συχνότητα","","","Hz","50","50","","50"]
["","Όνομα","","","","V1","V1","","V1"]
["","Τάση","","","V","220-240","220-240","","220-240"]
["Σημειώσεις","","","","","(1) - Όλες οι μονάδες ελέγχονται και συμμορφώνονται με το ISO5151 (μονάδα χωρίς αεραγωγό) ή ISO13253 (μονάδα με αεραγωγό)","(1) - Όλες οι μονάδες ελέγχονται και συμμορφώνονται με το ISO5151 (μονάδα χωρίς αεραγωγό) ή ISO13253 (μονάδα με αεραγωγό)","","(1) - Όλες οι μονάδες ελέγχονται και συμμορφώνονται με το ISO5151 (μονάδα χωρίς αεραγωγό) ή ISO13253 (μονάδα με αεραγωγό)"]
["","","","","","(2) - Όλες οι προδιαγραφές μπορεί να τροποποιηθούν από τον κατασκευαστή χωρίς προηγούμενη ειδοποίηση.","(2) - Όλες οι προδιαγραφές μπορεί να τροποποιηθούν από τον κατασκευαστή χωρίς προηγούμενη ειδοποίηση.","","(2) - Όλες οι προδιαγραφές μπορεί να τροποποιηθούν από τον κατασκευαστή χωρίς προηγούμενη ειδοποίηση."]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Ονομ.","m³/min","","","13.30"]
["","","Θέρμανση","Ονομ.","m³/min","","","13.30"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","","","1668"]
["","Θέρμανση","","Ονομ.","kW","","","1550"]
["Περίβλημα","Χρώμα","","","","","","Λευκό"]
["","Υλικό","","","","","","Πολυστυρένιο υψηλής αντοχής"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","","","310"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","","","1124"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","","","237"]
["Βάρος","Μονάδα","","","kg","","","14"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","","","15"]
["","","","Χαμηλή","m³/min","","","11.8"]
["","","","Αθόρυβη λειτουργία","m³/min","","","10.6"]
["","","Θέρμανση","Υψ.","m³/min","","","15.3"]
["","","","Χαμηλή","m³/min","","","11.8"]
["","","","Αθόρυβη λειτουργία","m³/min","","","10.6"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","","","55"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υπερ-υψηλό","dBA","","","44"]
["","","","Υψ.","dBA","","","40"]
["","","","Χαμηλή","dBA","","","35"]
["","","","Αθόρυβη λειτουργία","dBA","","","32"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","","12.7"]
["","Αποχέτευση","","","","","","16.5"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","","","1"]
["","Wireless remote control","","","","","","1"]
["","Titanium apatite filters","","","","","","Titanium apatite filters"]
["","Operation manual","","","","","","1"]
["","Batteries","","","","","","Batteries"]
["","Mounting plate","","","","","","1"]
["","Remote control holder","","","","","","1"]
["Τροφοδοσία ισχύος","Όνομα","","","","","","V1"]
["","Φάση","","","","","","1~"]
["","Συχνότητα","","","Hz","","","50"]
["","Τάση","","","V","","","220-240"]