{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-K3 / ARXP-K3"]
[]
[]
[]
[]
["","","","","ATXP20K3V1B / ARXP20K3V1B","ATXP25K3V1B / ARXP25K3V1B","ATXP35K3V1B / ARXP35K3V1B"]
["Απόδοση ψύξης","Ονομ.","","kW","","2.50","3.50"]
["Ονομαστική απόδοση","EER","","","","3.79","3.45"]
["","COP","","","","4.36","4.02"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","","A","A"]
["","","Θέρμανση","","","A","A"]
["Απόδοση θέρμανσης","Ονομ.","","kW","","3.00","4.00"]
["Σημειώσεις","","","","","(1) - Ψύξη: T2: εσωτ. θερμ. 26,6°CDB, 19,4°CWB, εξωτ. θερμ. 48°CDB [Btu/hr/W]","(1) - Ψύξη: T2: εσωτ. θερμ. 26,6°CDB, 19,4°CWB, εξωτ. θερμ. 48°CDB [Btu/hr/W]"]
["","","","","","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m.","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m."]
["","","","","","(3) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(3) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["Εξωτερική μονάδα","","","","ARXP20K3V1B"]
["Απόδοση ψύξης","Ονομ.","","kW","2.00"]
["Απόδοση θέρμανσης","Ονομ.","","kW","2.50"]
["Ονομαστική απόδοση","EER","","","3.98"]
["","COP","","","4.77"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A"]
["","","Θέρμανση","","A"]
["Ψύξη χώρου","Κατηγορία ενεργειακής αποδοτικότητας","","","A++"]
["","Απόδοση","Pdesign","kW","2.00"]
["","SEER","","","6.75"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","104"]
["Θέρμανση χώρου (Μέσο κλίμα)","Κατηγορία ενεργειακής αποδοτικότητας","","","A++"]
["","Απόδοση","Pdesign","kW","2.20"]
["","SCOP/A","","","4.64"]
["","Pdh Θερμαντική απόδοση στους -10°","","kW","2.19"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","664"]