{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BR00000678"]
[]
[]
[]
[]
["","","","","","BR00000678."]
["Εφαρμογή","","","","","Τύπου δαπέδου"]
["Απόδοση","m³/min","","","","33.33"]
["Περίβλημα","Χρώμα","","","","Βαμμένο γαλβανισμένο φινίρισμα χάλυβα"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","1628"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","720"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","770"]
["Βάρος","Μονάδα","","","kg","150"]
["Κατάλληλο εμβαδόν δωματίου","m²","","","","133"]
["Λειτουργία φιλτραρίσματος αέρα","Ισχύς εισόδου","","Υ","kW","0.379"]
["Στάθμη ηχητικής πίεσης","Λειτουργία φιλτραρίσματος αέρα","","Στάθμη ηχητικής πίεσης-=-Λειτουργία φιλτραρίσματος αέρα-=-Υψ.-=-dBA","dBA","55.9"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Λειτουργία φιλτραρίσματος αέρα","Turbo","m³/ώρα","2300"]
["","","","Υψ.","m³/ώρα","2000"]
["Διατάξεις ασφαλείας","Εξάρτημα","","01","","Διακόπτης ασφαλείας (η λειτουργία σταματά όταν ανοίξει η πίσω θύρα)"]
["Στάνταρτ εξαρτήματα","Prefilter selected","","","","1"]
["","HEPA filter selected","","","","1"]
["","Quick Start and Maintenance Guide","","","","1"]
["","Installation and Operation Manual available for download","","","","1"]
["Καλώδιο τροφοδοσίας","m","","","","3"]
["Τροφοδοσία ισχύος","Συχνότητα","","","Hz","50/60"]
["Ρεύμα λειτουργίας","Λειτουργία φιλτραρίσματος αέρα","","Υψ.","A","1.73"]