{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32 / 4MXM-A"]
[]
[]
[]
[]
["","","","","","CHYHBH05AAV32 / 4MXM68A2V1B","CHYHBH05AFV32 / 4MXM80A2V1B","CHYHBH05AAV32 / 4MXM80A2V1B","CHYHBH08AAV32 / 4MXM80A2V1B"]
["Θέρμανση ζεστού νερού χρήσης","Γενικά","","Δηλωμένο προφίλ φορτίου","","","XL"]
["","Μέσο κλίμα","","Κατηγορία ενεργειακής απόδοσης θέρμανσης νερού","","","A"]
["COP","","","","","3.91 (1)","4.04 (1)","4.04 (1)","4.17"]
["Θέρμανση χώρου","Εξαγωγή νερού μέσου κλίματος 55°C","Γενικά","Seasonal space heating eff. class","","","A+"]
["","","","ηs (Εποχιακή απόδοση θέρμανσης χώρου)","%","","120.8"]
["","","","SCOP","","","3.09"]
["Απόδοση θέρμανσης","Ονομ.","","","kW","","4.50 (1)"]
["Σημειώσεις","","","","","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), παράκαμψη μπόιλερ","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), παράκαμψη μπόιλερ","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), παράκαμψη μπόιλερ","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), παράκαμψη μπόιλερ"]
["Απόδοση θέρμανσης","Ονομ.","","","kW","4.5 (1)","","4.5 (1)","6.78"]
["Θέρμανση ζεστού νερού χρήσης","Γενικά","","Δηλωμένο προφίλ φορτίου","","XL","","XL","XL"]
["","Μέσο κλίμα","","Κατηγορία ενεργειακής απόδοσης θέρμανσης νερού","","A","","A","A"]
["Θέρμανση χώρου","Εξαγωγή νερού μέσου κλίματος 55°C","Γενικά","SCOP","","2.91","","3.09","3.09"]
["","","","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","A+","","A+","A+"]