{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Στάθμη ηχ. πίεσης","Θέρμανση","","Υψ.","dBA","38","","41"]
["","","","Αθόρυβη λειτουργία","dBA","21","","21"]
["","","","Χαμηλή","dBA","28","","30"]
["","Ψύξη","","Αθόρυβη λειτουργία","dBA","21","","21"]
["","","","Χαμηλή","dBA","25","","28"]
["","","","Υψ.","dBA","37","","42"]
["","","","Ονομ.","dBA","33"]
["","Ψύξη","","Ονομ.","dBA","31","","35"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης","","","","1","","1"]
["","Εγχειρίδιο χειρισμού","","","","1","","1"]
["","Ασύρματο τηλεχειριστήριο","","","","1","","1"]
["","Μπαταρίες","","","","2","","2"]
["","Υποδοχή τηλεχειριστηρίου","","","","1","","1"]
["","Πλάκα στήριξης","","","","1","","1"]
["","Βίδες στερέωσης εσωτερικής μονάδας","","","","2","","2"]
["","Φωτοκαταλυτικό φίλτρο αέρα από τιτάνιο με επικάλυψη απατίτη.","","","","2","","2"]
["Συστήματα ελέγχου","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Συνδέσεις σωληνώσεων","Υγρού","","ΕΞ.ΔΙΑΜ.","mm","6.35","","6.35"]
["","Αερίου","","ΕΞ.ΔΙΑΜ.","mm","9.5","","9.5"]
["","Συμπυκνωμάτων","","","","18","","18"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","0.040","","0.040"]
["","Θέρμανση","","Ονομ.","kW","0.040","","0.040"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","55","","59"]
["","Θέρμανση","","","dBA","56","","58"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","780","","780"]
["","","","Βάθος","mm","215","","215"]
["","","","Ύψος","mm","289","","289"]
["Casing","Colour","","","","Λευκό","","Λευκό"]
["Βάρος","Μονάδα","","","kg","8","","8"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Υψ.","m³/min","","","10.1"]
["","","","Χαμηλή","m³/min","","","6.3"]
["","","","Αθόρυβη λειτουργία","m³/min","","","4.3"]
["","","Ψύξη","Χαμηλή","m³/min","","","5.2"]
["","","","Υψ.","m³/min","","","9.2"]
["","","","Αθόρυβη λειτουργία","m³/min","","","3.9"]
["","","","Ονομ.","m³/min","","","8.1"]
["","","Ψύξη","Ονομ.","m³/min","","","7.2"]
["Power supply","Φάση","","","","1~","","1~"]
["","Συχνότητα","","","Hz","50","","50"]
["","Όνομα","","","","V1","","V1"]
["","Τάση","","","V","220-240","","220-240"]
["Σημειώσεις","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","","0.04","","0.040"]
["","Θέρμανση","","Ονομ.","kW","","0.04","","0.040"]
["Περίβλημα","Χρώμα","","","","","Λευκό","","Λευκό"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","","289","","289"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","","780","","780"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","","215","","215"]
["Βάρος","Μονάδα","","","kg","","8","","8.00"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","","7.9","","9.2"]
["","","","Μέτρια","m³/min","","6.3","","7.2"]
["","","","Χαμηλή","m³/min","","4.7","","5.2"]
["","","","Αθόρυβη λειτουργία","m³/min","","3.9","","3.9"]
["","","Θέρμανση","Υψ.","m³/min","","9","","10.1"]
["","","","Μέτρια","m³/min","","7.5","","8.1"]
["","","","Χαμηλή","m³/min","","6","","6.3"]
["","","","Αθόρυβη λειτουργία","m³/min","","4.3","","4.3"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","","55","","59"]
["","Θέρμανση","","","dBA","","56","","58"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","","37","","42"]
["","","","Μέτρια","dBA","","31","","35"]
["","","","Χαμηλή","dBA","","25","","28"]
["","","","Αθόρυβη λειτουργία","dBA","","21","","21"]
["","Θέρμανση","","Υψ.","dBA","","38","","41"]
["","","","Μέτρια","dBA","","33","","36"]
["","","","Χαμηλή","dBA","","28","","30"]
["","","","Αθόρυβη λειτουργία","dBA","","21","","21"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","6.35","","6.35"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","","9.5","","9.50"]
["","Αποχέτευση","","","","","18","","18"]
["Συστήματα ελέγχου","Infrared remote control","","","","","ARC466A6","","ARC466A6"]
["Στάνταρτ εξαρτήματα","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["Τροφοδοσία ισχύος","Όνομα","","","","","V1","","V1"]
["","Φάση","","","","","1~","","1~"]
["","Συχνότητα","","","Hz","","50","","50"]
["","Τάση","","","V","","220-240","","220-240"]