{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":11,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2CND-A4A"]
[]
[]
[]
[]
["","","","","","D2CND024A4AB","D2CND024A4AA","D2CND028A4AA","D2CND028A4AB","D2CND035A4AA","D2CND035A4AB"]
["Αέριο","Κατανάλωση (G20)","","Ελάχ.","m³/ώρα","0.31","0.31","0.511","0.511","0.511","0.511"]
["","","","Μέγ.","m³/ώρα","2.48","2.48","2.89","2.89","3.63","3.63"]
["","Κατανάλωση (G25)","","Ελάχ.","m³/ώρα","0.36","0.36","0.59","0.59","0.59","0.59"]
["","","","Μέγ.","m³/ώρα","2.89","2.89","3.32","3.32","4.19","4.19"]
["","Κατανάλωση (G31)","","Ελάχ.","m³/ώρα","0.12","0.12","0.2","0.2","0.2","0.2"]
["","","","Μέγ.","m³/ώρα","0.96","0.96","1.1","1.1","1.38","1.38"]
["","Κλάση NOx","","","","6","6","6","6","6","6"]
["","Επίπεδο NOx (G20)","","","mg/kWh","22","22","36.3","36.3","35.5","35.5"]
["Κεντρική θέρμανση","Qn εισόδου θερμότητας (κατώτερη θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","2.9","2.9","4.8","4.8","4.8","4.8"]
["","","","Μέγ.","kW","23.5","23.5","27","27","34","34"]
["","Qn εισόδου θερμότητας (μικτή θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","3.2","3.2","5.3","5.3","5.3","5.3"]
["","","","Μέγ.","kW","26.1","26.1","30","30","37.8","37.8"]
["","Pn εξόδου στους 80/60°C","","Ελάχ.","kW","2.8","2.8","4.6","4.6","4.6","4.6"]
["","","","Ονομ.","kW","22.8","22.8","26.3","26.3","33.2","33.2"]
["","Pnc εξόδου στους 50/30°C","","Ελάχ.","kW","3.1","3.1","5.2","5.2","5.2","5.2"]
["","","","Ονομ.","kW","24","24.0","28.2","28.2","35","35"]
["","Έξοδος στους 37/30°C","","Ονομ.","kW","7.6","7.6","8.8","8.8","11.1","11.1"]
["","Θερμοκρασία νερού","","Μέγ.","°C","100","100","100","100","100","100"]
["","Απόδοση","","Κατώτερη θερμαντική ισχύς","%","97.9","97.9"]
["","","","Μικτή θερμαντική ισχύς","%","87.3","87.3"]
["Ζεστό νερό χρήσης","Qnw εισόδου θερμότητας (κατώτερη θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","2.9","2.9","4.8","4.8","4.8","4.8"]
["","","","Μέγ.","kW","23.5","23.5","29.5","29.5","34","34"]
["","Qnw εισόδου θερμότητας (μικτή θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","3.2","3.2","5.3","5.3","5.3","5.3"]
["","","","Μέγ.","kW","26.1","26.1","32.7","32.7","37.7","37.7"]
["","Θερμοκρασία","","Μέγ.","°C","60","60","60","60","60","60"]
["Απώλειες θερμότητας","Ps μπόιλερ σε ετοιμότητα","","","kW","0.057","0.057","0.0650","0.065","0.0650","0.065"]
["Παροχή αέρα","Σύνδεση","","","mm","100","100","100","100","100","100"]
["","Ομόκεντρη","","","","Ναι","Ναι","Ναι","Ναι","Ναι","Ναι"]
["Απαέρια καύσης","Θερμοκρασία","","Μέγ.","°C","90","90","76.4","76.4","81.7","81.7"]
["","Σύνδεση","","","mm","60","60","60","60","60","60"]
["","Ροή μάζας (G20)","","Μέγ.","kg/h","38.7","38.7","44.5","55.7","55.7","55.7"]
["","Ροή μάζας (G31)","","Μέγ.","kg/h","36","36.0","43.3","43.3","54.7","54.7"]
["Περίβλημα","Χρώμα","","","","Λευκό τιτανίου (Ral9003)","Λευκό τιτανίου (Ral9003)","Λευκό τιτανίου (Ral9003)","Λευκό τιτανίου (Ral9003)","Λευκό τιτανίου (Ral9003)","Λευκό τιτανίου (Ral9003)"]
["","Υλικό","","","","Λαμαρίνα","Λαμαρίνα","Έλασμα από γαλβανισμένο χάλυβα με βαφή φούρνου","Έλασμα από γαλβανισμένο χάλυβα με βαφή φούρνου","Έλασμα από γαλβανισμένο χάλυβα με βαφή φούρνου","Έλασμα από γαλβανισμένο χάλυβα με βαφή φούρνου"]
["Διαστάσεις","Μονάδα","Ύψος","Περίβλημα","mm","590","590","690","690","690","690"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","400","400","440","440","440","440"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","256","256","295","295","295","295"]
["Βάρος","Μονάδα","","Κενό","kg","27","27","37","37","37","37"]
["","","","Πλήρες","kg","27","27","39","","39"]
["","Λέβητας","","Κενό","kg","27","27.0"]
["Θέρμανση ζεστού νερού χρήσης","Γενικά","","Δηλωμένο προφίλ φορτίου","","XL","XL","XL","XL","XL","XL"]
["","","","Κατηγορία ενεργειακής απόδοσης θέρμανσης νερού","","A","A","A","A","A","A"]
["Θέρμανση χώρου","Γενικά","","Κατηγορία απόδοσης εποχιακής θέρμανσης χώρου","","A","A","A","A","A","A"]
["Απαέρια καύσης","Ροή μάζας (G25)","","Μέγ.","kg/h","","","39.3","39.3","49.6","49.6"]