{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2CNL-A1A"]
[]
[]
[]
[]
["","","","","","D2CNL024A1AA"]
["Αέριο","Κατανάλωση (G20)","","Ελάχ.","m³/ώρα","0.40"]
["","","","Μέγ.","m³/ώρα","2.50"]
["","Κλάση NOx","","","","6"]
["","Επίπεδο NOx (G20)","","","mg/kWh","42"]
["Κεντρική θέρμανση","Qn εισόδου θερμότητας (κατώτερη θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","4.0"]
["","","","Μέγ.","kW","23.5"]
["","Qn εισόδου θερμότητας (μικτή θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","4.4"]
["","","","Μέγ.","kW","26.1"]
["","Pn εξόδου στους 80/60°C","","Ελάχ.","kW","3.8"]
["","","","Ονομ.","kW","22.8"]
["","Pnc εξόδου στους 50/30°C","","Ελάχ.","kW","4.4"]
["","","","Ονομ.","kW","24.0"]
["","Έξοδος στους 37/30°C","","Ονομ.","kW","4.4"]
["","Θερμοκρασία νερού","","Μέγ.","°C","100"]
["Ζεστό νερό χρήσης","Qnw εισόδου θερμότητας (κατώτερη θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","4.0"]
["","","","Μέγ.","kW","25.5"]
["","Qnw εισόδου θερμότητας (μικτή θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","4.4"]
["","","","Μέγ.","kW","28.3"]
["","Θερμοκρασία","","Μέγ.","°C","65"]
["Παροχή αέρα","Σύνδεση","","","mm","100"]
["","Ομόκεντρη","","","","Ναι"]
["Απαέρια καύσης","Θερμοκρασία","","Μέγ.","°C","81"]
["","Σύνδεση","","","mm","60"]
["","Ροή μάζας (G20)","","Μέγ.","kg/h","1.7"]
["Περίβλημα","Χρώμα","","","","Λευκό τιτανίου (Ral9003)"]
["","Υλικό","","","","Έλασμα από γαλβανισμένο χάλυβα με βαφή φούρνου"]
["Διαστάσεις","Μονάδα","Ύψος","Περίβλημα","mm","590"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","400"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","256"]
["Βάρος","Μονάδα","","Κενό","kg","27"]
["","","","Πλήρες","kg","31"]
["Θέρμανση ζεστού νερού χρήσης","Γενικά","","Δηλωμένο προφίλ φορτίου","","XL"]
["","","","Κατηγορία ενεργειακής απόδοσης θέρμανσης νερού","","A"]
["Θέρμανση χώρου","Γενικά","","Κατηγορία απόδοσης εποχιακής θέρμανσης χώρου","","A"]