{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EABH-D9W / EPGA011-016DV"]
[]
[]
[]
[]
["","","","","","EABH16DA9W / EPGA11DAV3","EABH16DF9W / EPGA11DAV3","EABH16DA9W / EPGA14DAV3","EABH16DF9W / EPGA14DAV3","EABH16DA9W / EPGA16DAV3","EABH16DF9W / EPGA16DAV3"]
["COP","","","","","5.15 (1), 3.88 (2)","5.15 (1), 3.88 (2)","4.99 (1), 3.65 (2)","4.99 (1), 3.65 (2)","4.78 (1), 3.71 (2)","4.78 (1), 3.71 (2)"]
["Εσωτερική μονάδα","","","","","EABH16DA9W","EABH16DA9W","EABH16DA9W","EABH16DA9W","EABH16DA9W","EABH16DA9W"]
["Θέρμανση χώρου","Εξαγωγή νερού μέσου κλίματος 55°C","Γενικά","Seasonal space heating eff. class","","A++","","A++","","A++"]
["","","","SCOP","","3.29","","3.34","","3.41"]
["","Εξαγωγή νερού μέσου κλίματος 35°C","Γενικά","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","A++","","A+++","","A+++"]
["","","","SCOP","","4.38","","4.45","","4.56"]
["Απόδοση θέρμανσης","Ονομ.","","","kW","11.1 (1), 11.3 (2)","","14.5 (1), 14.5 (2)","","16.5 (1), 15.6 (2)"]
["Ισχύς εισόδου","Θέρμανση","","Ονομ.","kW","2.16 (1), 2.91 (2)","","2.91 (1), 3.96 (2)","","3.45 (1), 4.21 (2)"]
["Σημειώσεις","","","","","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["Απόδοση θέρμανσης","Ονομ.","","","kW","","11.1 (1), 11.3 (2)","","14.5 (2) (1), 14.5 (2) (1)","","16.5 (1), 15.6 (2)"]
["Ισχύς εισόδου","Θέρμανση","","Ονομ.","kW","","2.16 (1), 2.91 (2)","","2.91 (1), 3.96 (2)","","3.45 (1), 4.21 (2)"]
["Θέρμανση χώρου","Εξαγωγή νερού μέσου κλίματος 55°C","Γενικά","SCOP","","","3.29","","3.34","","3.41"]
["","","","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","","A++","","A++","","A++"]
["","Εξαγωγή νερού μέσου κλίματος 35°C","Γενικά","SCOP","","","4.38","","4.45","","4.56"]
["","","","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","","A++","","A+++","","A+++"]
["Εύρος ενεργειακής αποδοτικότητας","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","","Space Heating A+++ ~ D, Water Heating A+ ~ F","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]