{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":11,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EABX-D6V / EPGA011-016DV"]
[]
[]
[]
[]
["","","","","","EABX16DA6V / EPGA11DAV3","EABX16DF6V / EPGA11DAV3","EABX16DA6V / EPGA14DAV3","EABX16DF6V / EPGA14DAV3","EABX16DA6V / EPGA16DAV3","EABX16DF6V / EPGA16DAV3"]
["COP","","","","","5.15 (1), 3.88 (2)","5.15 (1), 3.88 (2)","4.99 (1), 3.65 (2)","4.99 (1), 3.65 (2)","4.78 (1), 3.71 (2)","4.78 (1), 3.71 (2)"]
["Εσωτερική μονάδα","","","","","EABX16DA6V","EABX16DA6V","EABX16DA6V","EABX16DA6V","EABX16DA6V","EABX16DA6V"]
["Θέρμανση χώρου","Εξαγωγή νερού μέσου κλίματος 55°C","Γενικά","Seasonal space heating eff. class","","A++","","A++","","A++"]
["","","","SCOP","","3.32","","3.37","","3.43"]
["","Εξαγωγή νερού μέσου κλίματος 35°C","Γενικά","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","A+++","","A+++","","A+++"]
["","","","SCOP","","4.44","","4.51","","4.61"]
["Απόδοση ψύξης","Ονομ.","","","kW","10.5 (1), 10.7 (2)","10.5 (1), 10.7 (2)","11.1 (1), 11.9 (2)","","13.5 (1), 11.9 (2)"]
["EER","","","","","4.75 (1), 3.23 (2)","4.75 (1), 3.23 (2)","4.09 (1), 2.99 (2)","4.09 (1), 2.99 (2)","3.94 (1), 2.99 (2)","3.94 (1), 2.99 (2)"]
["Απόδοση θέρμανσης","Ονομ.","","","kW","11.1 (1), 11.3 (2)","11.1 (1), 11.3 (2)","14.5 (1), 14.5 (2)","","16.5 (1), 15.6 (2)"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","2.21 (1), 3.30 (2)","2.21 (1), 3.30 (2)","2.72 (1), 3.97 (2)","","3.42 (1), 3.97 (2)"]
["","Θέρμανση","","Ονομ.","kW","2.16 (1), 2.91 (2)","2.16 (1), 2.91 (2)","2.91 (1), 3.96 (2)","","3.45 (1), 4.21 (2)"]
["Σημειώσεις","","","","","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["Απόδοση θέρμανσης","Ονομ.","","","kW","","","","14.5 (1) (2), 14.5 (1) (2)","","16.5 (1), 15.6 (2)"]
["Απόδοση ψύξης","Ονομ.","","","kW","","","","11.1 (1), 11.9 (2)","","13.5 (1), 11.9 (2)"]
["Ισχύς εισόδου","Θέρμανση","","Ονομ.","kW","","","","2.91 (1), 3.96 (2)","","3.45 (1), 4.21 (2)"]
["","Ψύξη","","Ονομ.","kW","","","","2.72 (1), 3.97 (2)","","3.42 (1), 3.97 (2)"]
["Θέρμανση χώρου","Εξαγωγή νερού μέσου κλίματος 55°C","Γενικά","SCOP","","","","","3.37","","3.43"]
["","","","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","","","","A++","","A++"]
["","Εξαγωγή νερού μέσου κλίματος 35°C","Γενικά","SCOP","","","","","4.51","","4.61"]
["","","","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","","","","A+++","","A+++"]
["Εύρος ενεργειακής αποδοτικότητας","","","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]