{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":11,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EAVX-D9W / EPGA011-016DV"]
[]
[]
[]
[]
["","","","","","EAVX16S18DA9W / EPGA11DAV3","EAVX16S23DA9W / EPGA11DAV3","EAVX16S18DA9W / EPGA14DAV3","EAVX16S23DA9W / EPGA14DAV3","EAVX16S18DA9W / EPGA16DAV3","EAVX16S23DA9W / EPGA16DAV3"]
["Θέρμανση ζεστού νερού χρήσης","Γενικά","","Δηλωμένο προφίλ φορτίου","","L","","L","XL","L","XL"]
["","Μέσο κλίμα","","Κατηγορία ενεργειακής απόδοσης θέρμανσης νερού","","A","","A","A","A","A"]
["COP","","","","","5.15 (1), 3.88 (2)","5.15, 3.88","4.99 (1), 3.65 (2)","4.99 (1), 3.65 (2)","4.78 (1), 3.71 (2)","4.78 (1), 3.71 (2)"]
["Indoor unit","","","","","EAVX16S18DA9W","EAVX16S23DA9W","EAVX16S18DA9W","EAVX16S23DA9W","EAVX16S18DA9W","EAVX16S23DA9W"]
["Απόδοση ψύξης","Ονομ.","","","kW","10.5 (1), 10.7 (2)","","11.1 (1), 11.9 (2)","11.1 (1), 11.9 (2)","13.5 (1), 11.9 (2)","13.5 (1), 11.9 (2)"]
["EER","","","","","4.75 (1), 3.23 (2)","4.75, 3.23","4.09 (1), 2.99 (2)","4.09 (1), 2.99 (2)","3.94 (1), 2.99 (2)","3.94 (1), 2.99 (2)"]
["Απόδοση θέρμανσης","Ονομ.","","","kW","11.1 (1), 11.3 (2)","","14.5 (1), 14.5 (2)","14.5 (1), 14.5 (2)","16.5 (1), 15.6 (2)","16.5 (1), 15.6 (2)"]
["Ισχύς εισόδου","Ψύξη","","Ονομ.","kW","2.21 (1), 3.30 (2)","","2.72 (1), 3.97 (2)","2.72 (1), 3.97 (2)","3.42 (1), 3.97 (2)","3.42 (1), 3.97 (2)"]
["","Θέρμανση","","Ονομ.","kW","2.16 (1), 2.91 (2)","","2.91 (1), 3.96 (2)","2.91 (1), 3.96 (2)","3.45 (1), 4.21 (2)","3.45 (1), 4.21 (2)"]
["Σημειώσεις","","","","","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["Απόδοση θέρμανσης","Ονομ.","","","kW","","11.1, 11.3"]
["Απόδοση ψύξης","Ονομ.","","","kW","","10.5, 10.7"]
["Ισχύς εισόδου","Θέρμανση","","Ονομ.","kW","","2.16, 2.91"]
["","Ψύξη","","Ονομ.","kW","","2.21, 3.30"]
["","Ζεστό νερό χρήσης από 10°C έως 50°C","","Ονομ.","kWh","","3.08"]
["Χρόνος θέρμανσης από 10°C έως 50°C","hr","","","","","9 ώ 20 λεπτά σε θερμοκρασία περιβάλλοντος 7°C"]
["Θέρμανση ζεστού νερού χρήσης","Γενικά","","Δηλωμένο προφίλ φορτίου","","","XL"]
["","Μέσο κλίμα","","Κατηγορία ενεργειακής απόδοσης θέρμανσης νερού","","","A"]
["Θέρμανση χώρου","Εξαγωγή νερού μέσου κλίματος 55°C","Γενικά","SCOP","","","3.32"]
["","","","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","","A++"]
["","Εξαγωγή νερού μέσου κλίματος 35°C","Γενικά","SCOP","","","4.44"]
["","","","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","","A+++"]