{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":13,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSXB-D / ERLA-DW17"]
[]
[]
[]
[]
["","","","","","EBSXB16P30DF / ERLA16D2W17","EBSXB16P50DF / ERLA16D2W17","EBSXB16P30DF / ERLA16DAW17","EBSXB16P50DF / ERLA16DAW17","EBSXB16P50DG / ERLA16D2W17","EBSXB16P30DG / ERLA16DAW17","EBSXB16P30DG / ERLA16D2W17","EBSXB16P50DG / ERLA16DAW17"]
["Εσωτερική μονάδα","","","","","EBSXB16P30DF","EBSXB16P50DF","EBSXB16P30DF","EBSXB16P50DF","EBSXB16P50DG","EBSXB16P30DG","EBSXB16P30DG","EBSXB16P50DG"]
["Απόδοση θέρμανσης","Ονομ.","","","kW","16.0 (1)","16.0 (1)","16.0 (1)","16.0 (1)","16.0","16.0","16.0","16.0"]
["Απόδοση ψύξης","Ονομ.","","","kW","13.6 (2)","13.6 (2)","13.6 (2)","13.6 (2)","13.6 (2)","13.6 (2)","13.6 (2)","13.6 (2)"]
["Ισχύς εισόδου","Θέρμανση","","Ονομ.","kW","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)"]
["","Ψύξη","","Ονομ.","kW","4.68 (2)","4.68 (2)","4.68 (2)","4.68 (2)","4.68 (2)","4.68 (2)","4.68 (2)","4.68 (2)"]
["COP","","","","","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)"]
["EER","","","","","2.91 (2)","2.91 (2)","2.91 (2)","2.91 (2)","2.91 (2)","2.91 (2)","2.91 (2)","2.91 (2)"]
["Θέρμανση ζεστού νερού χρήσης","Γενικά","","Δηλωμένο προφίλ φορτίου","","L","XL","L","XL","XL","L","L","XL"]
["","Μέσο κλίμα","","Κατηγορία ενεργειακής απόδοσης θέρμανσης νερού","","A+","A+","A+","A+","A+","A+","A+","A+"]
["Θέρμανση χώρου","Εξαγωγή νερού μέσου κλίματος 55°C","Γενικά","SCOP","","3.35","3.35","3.35","3.35","3.35","3.35","3.35","3.35"]
["","","","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Εξαγωγή νερού μέσου κλίματος 35°C","Γενικά","SCOP","","4.68","4.68","4.68","4.68","4.68","4.68","4.68","4.68"]
["","","","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Σημειώσεις","","","","","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]