{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSQH-A9W"]
[]
[]
[]
[]
["","","","","","EGSQH10S18AA9W"]
["Στάθμη ηχητικής πίεσης","Ονομ.","","","dBA","32.0 (6)"]
["Ψυκτικό μέσο","GWP","","","","2,090"]
["","Φορτίο","","","kg","1.80"]
["","Τύπος","","","","R-410A"]
["Εύρος λειτουργίας","Χώρος εγκατάστασης","","Ελάχ.","°C","5.00"]
["","","","Μέγ.","°C","30.0"]
["","Θέρμανση","Πλευρά νερού","Μέγ.","°C","60.0 (7), 65.0 (8)"]
["","","","Min.","°C","24 (7), 24 (8)"]
["","Πλευρά άλμης","","Ελάχ.","°C","-5.00"]
["","","","Μέγ.","°C","20.0"]
["","Ζεστό νερό χρήσης","Πλευρά νερού","Μέγ.","°C","55 (7), 60 (9)"]
["","","","Ελάχ.","°C","25 (7), 25 (9)"]
["Ισχύς εισόδου","Nom.","","","kW","2.38 (1), 2.89 (2)"]
["Sound power level","Nom.","","","dBA","46.0"]
["COP","","","","","4.33 (1), 3.18 (2)"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","600"]
["","","","Βάθος","mm","728"]
["","","","Ύψος","mm","1,730"]
["Περίβλημα","Υλικό","","","","Λαμαρίνα με επικάλυψη"]
["","Χρώμα","","","","Λευκό"]
["Δεξαμενή","Όγκος νερού","","","l","180"]
["","Προστασία από τη διάβρωση","","","","Άνοδος"]
["","Μόνωση","","Απώλεια θερμότητες","kWh/24ωρ","1.36 (4)"]
["Βάρος","Μονάδα","","","kg","210"]
["Θέρμανση χώρου","Εξαγωγή νερού μέσου κλίματος 35°C","Γενικά","ηs (Εποχιακή απόδοση θέρμανσης χώρου)","%","194"]
["","","","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","A+++"]
["","","","SCOP","","5.06"]
["","Εξαγωγή νερού μέσου κλίματος 55°C","Γενικά","Seasonal space heating eff. class","","A++"]
["","","","ηs (Εποχιακή απόδοση θέρμανσης χώρου)","%","139"]
["","","","SCOP","","3.68"]
["Απόδοση θέρμανσης","Ονομ.","","","kW","10.3 (1), 9.20 (2)"]
["","Ελάχ.","","","kW","3.11 (1), 2.47 (2)"]
["","Μέγ.","","","kW","13.0 (1), 11.9 (2)"]
["Power supply","Φάση","","","","3~"]
["","Όνομα","","","","9W"]
["","Συχνότητα","","","Hz","50"]
["","Τάση","","","V","400"]
["Ρεύμα","Συνιστώμενες ασφάλειες","","","A","25"]
["Σημειώσεις","","","","","(1) - EWB/LWB 0°C/-3°C - LWC 35°C (DT=5°C)"]
["","","","","","(2) - EWB/LWB 0°C/-3°C - LWC 45°C (DT=5°C)"]
["","","","","","(3) - με 40% προπυλενογλυκόλη"]
["","","","","","(4) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897"]
["","","","","","(5) - συμπεριλαμβανομένων σωληνώσεων + PHE + εφεδρικός θερμαντήρας / εξαιρείται το δοχείο διαστολής"]
["","","","","","(6) - Η στάθμη ηχητικής πίεσης μετράται με μικρόφωνο σε απόσταση 1m από τη μονάδα. Είναι μία σχετική τιμή που εξαρτάται από την απόσταση και το ακουστικό περιβάλλον."]
["","","","","","(7) - Με αντλία θερμότητας"]
["","","","","","(8) - Με αντλία θερμότητας + εφεδρικό θερμαντήρα"]
["","","","","","(9) - Με εφεδρικό θερμαντήρα"]