{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSHB-D3"]
[]
[]
[]
[]
["","","","","","EHSHB04P30DA3","EHSHB08P30DA3","EHSHB08P50DA3"]
["Περίβλημα","Χρώμα","","","","Χρώμα Traffic white (RAL9016) / Σκούρο γκρι (RAL7011)","Χρώμα Traffic white (RAL9016) / Σκούρο γκρι (RAL7011)","Χρώμα Traffic white (RAL9016) / Σκούρο γκρι (RAL7011)"]
["","Υλικό","","","","Πολυπροπυλένιο με αντοχή στις κρούσεις","Πολυπροπυλένιο με αντοχή στις κρούσεις","Πολυπροπυλένιο με αντοχή στις κρούσεις"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","1891","1891","1896"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","595","595","790"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","615","615","790"]
["Βάρος","Μονάδα","","","kg","76.0","76.0","99.0"]
["PED","Κατηγορία","","","","Είδος 3.3","Είδος 3.3","Είδος 3.3"]
["Ψυκτικό μέσο","Τύπος","","","","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0"]
["","Φορτίο","","","kg","1.50","1.50","1.50"]
["Στάθμη ηχητικής ισχύος","Ονομ.","","","dBA","39","39","39"]
["Εύρος λειτουργίας","Θέρμανση","Πλευρά νερού","Ελάχ.","°C","18","18","18"]
["","","","Μέγ.","°C","65","65","65"]
["","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","10","10","10"]
["","","Πλευρά νερού","Ελάχ.","°C","5","5","5"]
["","","","Μέγ.","°C","22","22","22"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~","1~"]
["","Συχνότητα","","","Hz","50","50","50"]
["","Τάση","","","V","230","230","230"]
["Ηλεκτρικός θερμαντήρας","Τροφοδοσία ισχύος","","Όνομα","","3V / 9W","3V / 9W","3V / 9W"]
["","","","Φάση","","1~ / 3~","1~ / 3~","1~ / 3~"]
["","","","Συχνότητα","Hz","50","50","50"]
["Σημειώσεις","","","","","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]
["","","","","","","","(5) - Θέρμανση δοχείου μόνο με αντλία θερμ., όχι ηλ. θερμαντήρα"]