{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":9,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSXB-E / ERGA-EV7"]
[]
[]
[]
[]
["","","","","","EHSXB04P30EF / ERGA04EAV37","EHSXB04P50EF / ERGA04EAV37","EHSXB04P50EG / ERGA04EAV37","EHSXB04P30EG / ERGA04EAV37"]
["Εσωτερική μονάδα","","","","","EHSXB04P30EF","EHSXB04P50EF","EHSXB04P50EG","EHSXB04P30EG"]
["Απόδοση θέρμανσης","Ονομ.","","","kW","4.36 (1), 4.60 (2)","4.36 (1), 4.60 (2)","4.36 (1), 4.60 (2)","4.36 (1), 4.60 (2)"]
["Απόδοση ψύξης","Ονομ.","","","kW","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)"]
["Ισχύς εισόδου","Θέρμανση","","Ονομ.","kW","0.830 (1), 1.26 (2)","0.830 (1), 1.26 (2)","0.830 (1), 1.26 (2)","0.830 (1), 1.26 (2)"]
["","Ψύξη","","Ονομ.","kW","0.810 (1), 1.36 (2)","0.810 (1), 1.36 (2)","0.810 (1), 1.36 (2)","0.810 (1), 1.36 (2)"]
["COP","","","","","5.23 (1), 3.65 (2)","5.23 (1), 3.65 (2)","5.23 (1), 3.65 (2)","5.23 (1), 3.65 (2)"]
["EER","","","","","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)"]
["Θέρμανση ζεστού νερού χρήσης","Γενικά","","Δηλωμένο προφίλ φορτίου","","L","XL","XL","L"]
["","Μέσο κλίμα","","Κατηγορία ενεργειακής απόδοσης θέρμανσης νερού","","A+","A+","A+","A+"]
["Θέρμανση χώρου","Εξαγωγή νερού μέσου κλίματος 55°C","Γενικά","SCOP","","3.29","3.29","3.29","3.29"]
["","","","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","A++","A++","A++","A++"]
["","Εξαγωγή νερού μέσου κλίματος 35°C","Γενικά","SCOP","","4.96","4.96","4.96","4.96"]
["","","","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","A+++","A+++","A+++","A+++"]
["Εύρος ενεργειακής αποδοτικότητας","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Σημειώσεις","","","","","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]