{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":9,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVZ-E9W / ERGA-EVH7"]
[]
[]
[]
[]
["","","","","","EHVZ08S18EA9W / ERGA08EAV3H7","EHVZ08S18EJ9W / ERGA08EAV3H7","EHVZ08S23EA9W / ERGA08EAV3H7","EHVZ08S23EJ9W / ERGA08EAV3H7"]
["Απόδοση θέρμανσης","Ονομ.","","","kW","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)"]
["Ισχύς εισόδου","Θέρμανση","","Ονομ.","kW","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)"]
["","Ζεστό νερό χρήσης από 10°C έως 50°C","","Ονομ.","kWh","2.48","2.48","3.01","3.01"]
["Χρόνος θέρμανσης από 10°C έως 50°C","hr","","","","1 ώρα 28 λεπτά","1 ώρα 28 λεπτά","1 ώρα 40 λεπτά","1 ώρα 40 λεπτά"]
["COP","","","","","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)"]
["Θέρμανση ζεστού νερού χρήσης","Γενικά","","Δηλωμένο προφίλ φορτίου","","L","L","XL","XL"]
["","Μέσο κλίμα","","Κατηγορία ενεργειακής απόδοσης θέρμανσης νερού","","A+","A+","A+","A+"]
["Θέρμανση χώρου","Εξαγωγή νερού μέσου κλίματος 55°C","Γενικά","SCOP","","3.32","3.32","3.32","3.32"]
["","","","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","A++","A++","A++","A++"]
["","Εξαγωγή νερού μέσου κλίματος 35°C","Γενικά","SCOP","","4.56","4.56","4.56","4.56"]
["","","","Κατηγορία εποχιακής απόδοσης θέρμανσης χώρου","","A+++","A+++","A+++","A+++"]
["Εύρος ενεργειακής αποδοτικότητας","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Σημειώσεις","","","","","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Συνθήκη 1: ψύξη Ta 35°C - LWE 18°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Συνθήκη 2: ψύξη Ta 35°C - LWE 7°C (DT = 5°C) θέρμανση Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]