{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":6,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWCB-B"]
[]
[]
[]
[]
["","","","","","EKHWCB500BA"]
["Στερέωση","","","","","Δάπεδο"]
["Περίβλημα","Χρώμα","","","","Χρώμα Traffic white (RAL9016) / Σκούρο γκρι (RAL7011)"]
["","Υλικό","","","","Πολυπροπυλένιο με αντοχή στις κρούσεις"]
["Διαστάσεις","Μονάδα","Ύψος","Δεξαμενή","mm","1,660"]
["","","","Πλάτος","mm","790"]
["","","","Βάθος","mm","790"]
["Βάρος","Μονάδα","","Κενό","kg","80"]
["","","","Πλήρες","kg","580"]
["Δεξαμενή","Όγκος νερού","","","l","477"]
["","Υλικό","","","","Πολυπροπυλένιο"]
["","Μέγιστη θερμοκρασία νερού","","","°C","85"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","","B"]
["Εναλλάκτης θερμότητας","Ζεστό νερό χρήσης","","Ποσότητα","","1"]
["","","","Υλικό σωλήνα","","Ανοξείδωτος χάλυβας (DIN 1,4404)"]
["","","","Όγκος εσωτερικής σερπαντίνας","l","25.8"]
["","","","Πίεση λειτουργίας","bar","6"]
["","","","Μέση συγκεκριμένη θερμική απόδοση","W/K","2,580"]
["","Φόρτιση","","Ποσότητα","","1"]
["","","","Υλικό σωλήνα","","Ανοξείδωτος χάλυβας (DIN 1,4404)"]
["","","","Όγκος εσωτερικής σερπαντίνας","l","9"]
["","","","Πίεση λειτουργίας","bar","3"]
["","","","Μέση συγκεκριμένη θερμική απόδοση","W/K","1,030"]
["","Βοηθητική ηλιακή θέρμανση","","Ποσότητα","","1"]
["","","","Υλικό σωλήνα","","Ανοξείδωτος χάλυβας (DIN 1,4404)"]
["","","","Όγκος εσωτερικής σερπαντίνας","l","4"]
["","","","Πίεση λειτουργίας","bar","3"]
["","","","Μέση συγκεκριμένη θερμική απόδοση","W/K","350"]
["Σημειώσεις","","","","","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]
["","","","","","(5) - Για όγκο κατανάλωσης 140l -> 5820 Wh (μπάνιο) / αντλία θερμότητας 8kW"]
["","","","","","(6) - Για όγκο κατανάλωσης 90l -> 3660 Wh (μπάνιο) / αντλία θερμότητας 8kW"]
["","","","","","(7) - Για όγκο κατανάλωσης 140l -> 5820 Wh (μπάνιο) / αντλία θερμότητας 16kW"]
["","","","","","(8) - Για όγκο κατανάλωσης 90l -> 3660 Wh (μπάνιο) / αντλία θερμότητας 16kW"]