{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":7,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWP-PB"]
[]
[]
[]
[]
["","","","","","EKHWP300PB","EKHWP500PB"]
["Στερέωση","","","","","Δάπεδο","Δάπεδο"]
["Περίβλημα","Χρώμα","","","","Χρώμα Traffic white (RAL9016) / Σκούρο γκρι (RAL7011)","Χρώμα Traffic white (RAL9016) / Σκούρο γκρι (RAL7011)"]
["","Υλικό","","","","Πολυπροπυλένιο με αντοχή στις κρούσεις","Πολυπροπυλένιο με αντοχή στις κρούσεις"]
["Διαστάσεις","Μονάδα","Ύψος","Δεξαμενή","mm","1646","1658"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","","790"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","","790"]
["Βάρος","Μονάδα","","Κενό","kg","56","82"]
["","","","Πλήρες","kg","350","559"]
["Δεξαμενή","Όγκος νερού","","","l","294","477"]
["","Υλικό","","","","Πολυπροπυλένιο","Πολυπροπυλένιο"]
["","Μέγιστη θερμοκρασία νερού","","","°C","85","85"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","","B","B"]
["Εναλλάκτης θερμότητας","Ζεστό νερό χρήσης","","Ποσότητα","","1","1"]
["","","","Υλικό σωλήνα","","Ανοξείδωτος χάλυβας (DIN 1.4404)","Ανοξείδωτος χάλυβας (DIN 1.4404)"]
["","","","Όγκος εσωτερικής σερπαντίνας","l","27.8","29.0"]
["","","","Πίεση λειτουργίας","bar","10.0","10.0"]
["","Φόρτιση","","Ποσότητα","","1","1"]
["","","","Υλικό σωλήνα","","Ανοξείδωτος χάλυβας (DIN 1.4404)","Ανοξείδωτος χάλυβας (DIN 1.4404)"]
["","","","Όγκος εσωτερικής σερπαντίνας","l","12.9","18.1"]
["","","","Πίεση λειτουργίας","bar","6.0","6.0"]
["","Βοηθητική ηλιακή θέρμανση","","Ποσότητα","","","1"]
["","","","Υλικό σωλήνα","","","Ανοξείδωτος χάλυβας (DIN 1.4404)"]
["","","","Όγκος εσωτερικής σερπαντίνας","l","","3.9"]
["","","","Πίεση λειτουργίας","bar","","3.0"]
["Σημειώσεις","","","","","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]
["","","","","","(5) - Για όγκο κατανάλωσης 140l -> 5820 Wh (μπάνιο) / αντλία θερμότητας 8kW","(5) - Για όγκο κατανάλωσης 140l -> 5820 Wh (μπάνιο) / αντλία θερμότητας 16kW"]
["","","","","","(6) - Για όγκο κατανάλωσης 90l -> 3660 Wh (μπάνιο) / αντλία θερμότητας 8kW","(6) - Για όγκο κατανάλωσης 90l -> 3660 Wh (μπάνιο) / αντλία θερμότητας 16kW"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","595"]
["","","","Βάθος","mm","615"]
["Εύρος ενεργειακής αποδοτικότητας","","","","","A+ ~ F"]
["Σημειώσεις","","","","","(7) - Για όγκο κατανάλωσης 140l -> 5820 Wh (μπάνιο) / αντλία θερμότητας 16kW"]
["","","","","","(8) - Για όγκο κατανάλωσης 90l -> 3660 Wh (μπάνιο) / αντλία θερμότητας 16kW"]
["","","","","","(9) - Εναλλάκτης  θερμότητας συνδεδεμένο παράλληλα, TKW= 10°C/ TWW= 45°C/ TSP= 65°C/ Pload= 35kW/ Tflow= 80°C"]
["","","","","","(10) - TKW= 10°C/ TWW= 45°C/ TSP= 65°C/ Pload= 35kW/ Tflow= 80°C"]