{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":8,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKOMB-AH"]
[]
[]
[]
[]
["","","","","","EKOMB22AAV1H","EKOMB28AAV1H","EKOMB33AAV1H"]
["Ζεστό νερό χρήσης","Qnw εισόδου θερμότητας (μικτή θερμαντική ισχύς)","Ονομ.","Μέγ.","kW","24.6","31.1","36.3"]
["","","","Ελάχ.","kW","6.2","7.9","8.0"]
["","Κατηγορία άνεσης (ΕΝ13203)","","","","L","XL","XL"]
["","Θερμοκρασία","","Μέγ.","°C","65","65","65"]
["","Qnw εισόδου θερμότητας (κατώτερη θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","5.6","7.1","7.2"]
["","","","Μέγ.","kW","22.1","28.0","32.7"]
["Απαέρια καύσης","Θερμοκρασία","","Μέγ.","°C","90","90","90"]
["","Ροή μάζας (G31)","","Μέγ.","kg/h","36.4","46.1","54.4"]
["Παροχή αέρα","Ομόκεντρη","","","","60/100","60/100","60/100"]
["Θέρμανση ζεστού νερού χρήσης","Γενικά","","Κατηγορία ενεργειακής απόδοσης θέρμανσης νερού","","A","A","A"]
["","","","Δηλωμένο προφίλ φορτίου","","L","XL","XL"]
["Διαστάσεις","Μονάδα","Ύψος","Περίβλημα","mm","590","650","710"]
["Περίβλημα","Υλικό","","","","Λαμαρίνα με επικάλυψη","Λαμαρίνα με επικάλυψη","Λαμαρίνα με επικάλυψη"]
["","Χρώμα","","","","RAL9010","RAL9010","RAL9010"]
["Θέρμανση χώρου","Γενικά","","Κατηγορία απόδοσης εποχιακής θέρμανσης χώρου","","A","A","A"]
["","","","ηs (Εποχιακή απόδοση θέρμανσης χώρου)","%","91","92","93"]
["Κεντρική θέρμανση","Qn εισόδου θερμότητας (μικτή θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","6.2","7.9","8.0"]
["","","","Μέγ.","kW","20.8","26.3","30.3"]
["","Θερμοκρασία νερού","","Μέγ.","°C","90","90","90"]
["","Pn εξόδου στους 80/60°C","","Ονομ.","kW","17.8","22.8","26.3"]
["","Qn εισόδου θερμότητας (κατώτερη θερμαντική ισχύς)","Ονομ.","Μέγ.","kW","18.7","23.7","27.3"]
["","","","Ελάχ.","kW","5.6","7.1","7.2"]
["Αέριο","Σύνδεση","","Διάμετρος","mm","15","15","15"]
["","Κατανάλωση (G31)","","Ελάχ.","m³/ώρα","0.22","0.28","0.28"]
["","","","Μέγ.","m³/ώρα","0.87","1.11","1.29"]
["","Κλάση NOx","","","","6","6","6"]