{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":70,"n_cols":8,"rows_kept":70,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKOMB-AH"]
[]
[]
[]
[]
["","","","","","EKOMB22AAV1H","EKOMB28AAV1H","EKOMB33AAV1H"]
["Ζεστό νερό χρήσης","Qnw εισόδου θερμότητας (μικτή θερμαντική ισχύς)","Ονομ.","Μέγ.","kW","","31.1"]
["","","","Ελάχ.","kW","","7.9"]
["","Κατηγορία άνεσης (ΕΝ13203)","","","","","XL"]
["","Θερμοκρασία","","Μέγ.","°C","","65"]
["","Qnw εισόδου θερμότητας (κατώτερη θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","","7.1"]
["","","","Μέγ.","kW","","28.0"]
["Απαέρια καύσης","Θερμοκρασία","","Μέγ.","°C","","90"]
["","Ροή μάζας (G31)","","Μέγ.","kg/h","","46.1"]
["Παροχή αέρα","Ομόκεντρη","","","","","60/100"]
["Θέρμανση ζεστού νερού χρήσης","Γενικά","","Κατηγορία ενεργειακής απόδοσης θέρμανσης νερού","","","A"]
["","","","Δηλωμένο προφίλ φορτίου","","","XL"]
["Διαστάσεις","Μονάδα","Ύψος","Περίβλημα","mm","","650"]
["Περίβλημα","Υλικό","","","","","Λαμαρίνα με επικάλυψη"]
["","Χρώμα","","","","","RAL9010"]
["Θέρμανση χώρου","Γενικά","","Κατηγορία απόδοσης εποχιακής θέρμανσης χώρου","","","A"]
["","","","ηs (Εποχιακή απόδοση θέρμανσης χώρου)","%","","92"]
["Κεντρική θέρμανση","Qn εισόδου θερμότητας (μικτή θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","","7.9"]
["","","","Μέγ.","kW","","26.3"]
["","Θερμοκρασία νερού","","Μέγ.","°C","","90"]
["","Pn εξόδου στους 80/60°C","","Ονομ.","kW","","22.8"]
["","Qn εισόδου θερμότητας (κατώτερη θερμαντική ισχύς)","Ονομ.","Μέγ.","kW","","23.7"]
["","","","Ελάχ.","kW","","7.1"]
["Αέριο","Σύνδεση","","Διάμετρος","mm","","15"]
["","Κατανάλωση (G31)","","Ελάχ.","m³/ώρα","","0.28"]
["","","","Μέγ.","m³/ώρα","","1.11"]
["","Κλάση NOx","","","","","6"]
["Αέριο","Σύνδεση","","Διάμετρος","mm","15","","15"]
["","Κατανάλωση (G20)","","Ελάχ.","m³/ώρα","0.58","","0.75"]
["","","","Μέγ.","m³/ώρα","2.29","","3.39"]
["","Κατανάλωση (G25)","","Ελάχ.","m³/ώρα","0.67","","0.86"]
["","","","Μέγ.","m³/ώρα","2.65","","3.93"]
["","Κατανάλωση (G31)","","Ελάχ.","m³/ώρα","0.22","","0.28"]
["","","","Μέγ.","m³/ώρα","0.87","","1.29"]
["","Κλάση NOx","","","","6","","6"]
["","Επίπεδο NOx (G20)","","","mg/kWh","33","","34"]
["Κεντρική θέρμανση","Qn εισόδου θερμότητας (κατώτερη θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","5.6","","7.2"]
["","","","Μέγ.","kW","18.7","","27.3"]
["","Qn εισόδου θερμότητας (μικτή θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","6.2","","8.0"]
["","","","Μέγ.","kW","20.8","","30.3"]
["","Pn εξόδου στους 80/60°C","","Ονομ.","kW","17.8","","26.3"]
["","Έξοδος στους 37/30°C","","Ονομ.","kW","6.0","","7.8"]
["","Θερμοκρασία νερού","","Μέγ.","°C","90","","90"]
["Ζεστό νερό χρήσης","Qnw εισόδου θερμότητας (κατώτερη θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","5.6","","7.2"]
["","","","Μέγ.","kW","22.1","","32.7"]
["","Qnw εισόδου θερμότητας (μικτή θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","6.2","","8.0"]
["","","","Μέγ.","kW","24.6","","36.3"]
["","Κατηγορία άνεσης (ΕΝ13203)","","","","L","","XL"]
["","Θερμοκρασία","","Μέγ.","°C","65","","65"]
["Παροχή αέρα","Ομόκεντρη","","","","όχι","","όχι"]
["Απαέρια καύσης","Θερμοκρασία","","Μέγ.","°C","90","","90"]
["","Σύνδεση","","","mm","60","","60"]
["","Ροή μάζας (G20)","","Μέγ.","kg/h","37.1","","53.6"]
["","Ροή μάζας (G25)","","Μέγ.","kg/h","37.1","","53.6"]
["","Ροή μάζας (G31)","","Μέγ.","kg/h","36.4","","54.4"]
["Περίβλημα","Χρώμα","","","","RAL9010","","RAL9010"]
["","Υλικό","","","","Λαμαρίνα με επικάλυψη","","Λαμαρίνα με επικάλυψη"]
["Διαστάσεις","Μονάδα","Ύψος","Περίβλημα","mm","590","","710"]
["","","","Πλάτος","mm","450","","450"]
["","","","Βάθος","mm","240","","240"]
["Βάρος","Μονάδα","","Κενό","kg","30","","36"]
["Θέρμανση ζεστού νερού χρήσης","Γενικά","","Δηλωμένο προφίλ φορτίου","","L","","XL"]
["","","","Κατηγορία ενεργειακής απόδοσης θέρμανσης νερού","","A","","A"]
["Θέρμανση χώρου","Γενικά","","Κατηγορία απόδοσης εποχιακής θέρμανσης χώρου","","A","","A"]
["Εύρος ενεργειακής αποδοτικότητας","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]