{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":11,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKOMBG-A"]
[]
[]
[]
[]
["","","","","","EKOMBG22AAV1","EKOMBG22ABV1","EKOMBG28AAV1","EKOMBG28ABV1","EKOMBG33AAV1","EKOMBG33ABV1"]
["Αέριο","Σύνδεση","","Διάμετρος","mm","15","15","15","15","15","15"]
["","Κατανάλωση (G20)","","Ελάχ.","m³/ώρα","0.58","0.58","0.74","0.74","0.79","0.79"]
["","","","Μέγ.","m³/ώρα","2.42","2.42","3.02","3.02","3.39","3.39"]
["","Κατανάλωση (G25)","","Ελάχ.","m³/ώρα","0.62","0.62","0.84","0.84","0.89","0.89"]
["","","","Μέγ.","m³/ώρα","2.82","2.82","3.46","3.46","3.92","3.92"]
["","Κατανάλωση (G31)","","Ελάχ.","m³/ώρα","0.21","0.21","0.29","0.29","0.30","0.30"]
["","","","Μέγ.","m³/ώρα","0.94","0.94","1.19","1.19","1.29","1.29"]
["","Κλάση NOx","","","","6","6","6","6","6","6"]
["","Επίπεδο NOx (G20)","","","mg/kWh","28","28","27","27","36","36"]
["Κεντρική θέρμανση","Qn εισόδου θερμότητας (κατώτερη θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","5.5","5.5","7.1","7.1","7.6","7.6"]
["","","","Μέγ.","kW","23.3","23.3","29.1","29.1","32.7","32.7"]
["","Qn εισόδου θερμότητας (μικτή θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","6.1","6.1","7.9","7.9","8.4","8.4"]
["","","","Μέγ.","kW","25.9","25.9","32.3","32.3","36.3","36.3"]
["","Pn εξόδου στους 80/60°C","","Ελάχ.","kW","6.0","6.0","7.6","7.6","8.3","8.3"]
["","","","Ονομ.","kW","22.6","22.6","28.2","28.2","32.0","32.0"]
["","Έξοδος στους 37/30°C","","Ονομ.","kW","6.0","6.0","7.6","7.6","8.3","8.3"]
["","Θερμοκρασία νερού","","Μέγ.","°C","90","90","90","90","90","90"]
["Ζεστό νερό χρήσης","Qnw εισόδου θερμότητας (κατώτερη θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","5.5","5.5","7.1","7.1","7.6","7.6"]
["","","","Μέγ.","kW","23.3","23.3","29.1","29.1","32.7","32.7"]
["","Qnw εισόδου θερμότητας (μικτή θερμαντική ισχύς)","Ονομ.","Ελάχ.","kW","6.1","6.1","7.9","7.9","8.4","8.4"]
["","","","Μέγ.","kW","25.9","25.9","23.3","23.3","36.3","36.3"]
["","Κατηγορία άνεσης (ΕΝ13203)","","","","L","L","XL","XL","XL","XL"]
["","Θερμοκρασία","","Μέγ.","°C","65","65","65","65","65","65"]
["Παροχή αέρα","Ομόκεντρη","","","","όχι","όχι","όχι","όχι","όχι","όχι"]
["Απαέρια καύσης","Θερμοκρασία","","Μέγ.","°C","70","70","70","70","70","70"]
["","Σύνδεση","","","mm","60","60","60","60","60","60"]
["","Ροή μάζας (G20)","","Μέγ.","kg/h","38.9","38.9","48.6","48.6","54.4","54.4"]
["","Ροή μάζας (G25)","","Μέγ.","kg/h","38.9","38.9","48.6","48.6","54.4","54.4"]
["","Ροή μάζας (G31)","","Μέγ.","kg/h","38.2","38.2","47.9","47.9","53.6","53.6"]
["Περίβλημα","Χρώμα","","","","RAL9010","RAL9010","RAL9010","RAL9010","RAL9010","RAL9010"]
["","Υλικό","","","","Λαμαρίνα με επικάλυψη","Λαμαρίνα με επικάλυψη","Λαμαρίνα με επικάλυψη","Λαμαρίνα με επικάλυψη","Λαμαρίνα με επικάλυψη","Λαμαρίνα με επικάλυψη"]
["Διαστάσεις","Μονάδα","Ύψος","Περίβλημα","mm","590","590","650","650","710","710"]
["","","","Πλάτος","mm","450","450","450","450","450","450"]
["","","","Βάθος","mm","240","240","240","240","240","240"]
["Βάρος","Μονάδα","","Κενό","kg","30","30","33","33","36","36"]
["Θέρμανση ζεστού νερού χρήσης","Γενικά","","Δηλωμένο προφίλ φορτίου","","L","L","XL","XL","XL","XL"]
["","","","Κατηγορία ενεργειακής απόδοσης θέρμανσης νερού","","A","A","A","A","A","A"]
["Θέρμανση χώρου","Γενικά","","Κατηγορία απόδοσης εποχιακής θέρμανσης χώρου","","A","A","A","A","A","A"]
["Εύρος ενεργειακής αποδοτικότητας","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]