{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":8,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKVDX-A"]
[]
[]
[]
[]
["","","","","EKVDX32A2VEB","EKVDX50A2VEB","EKVDX80A2VEB","EKVDX100A2VEB"]
["Εύρος λειτουργίας","Γύρω από τη μονάδα","","°CDB","10°C~40°CDB, σχ. υγρ. 80% ή λιγότερο","10°C~40°CDB, σχ. υγρ. 80% ή λιγότερο","10°C~40°CDB, σχ. υγρ. 80% ή λιγότερο","10°C~40°CDB, σχ. υγρ. 80% ή λιγότερο"]
["Βάρος","Μονάδα","","kg","19.0","23.4","30.1","37.7"]
["Ψυκτικό μέσο","Έλεγχος","","","Ηλεκτροκίνητη θερμοεκτονωτική βαλβίδα","Ηλεκτροκίνητη θερμοεκτονωτική βαλβίδα","Ηλεκτροκίνητη θερμοεκτονωτική βαλβίδα","Ηλεκτροκίνητη θερμοεκτονωτική βαλβίδα"]
["","GWP","","","675.0, 2,087.5","675.0, 2,087.5","675.0, 2,087.5","675.0, 2,087.5"]
["","Τύπος","","","R32/R410A","R32/R410A","R32/R410A","R32/R410A"]
["Συνδέσεις σωληνώσεων","Υγρό","ΕΞ.ΔΙΑΜ.","mm","6.35","6.35","6.35","6.35"]
["","","Τύπος","","Σύνδεση με εκχείλωση","Σύνδεση με εκχείλωση","Σύνδεση με εκχείλωση","Σύνδεση με εκχείλωση"]
["","Αέριο","ΕΞ.ΔΙΑΜ.","mm","12.7","12.7","12.7","12.7"]
["","","Τύπος","","Σύνδεση με εκχείλωση","Σύνδεση με εκχείλωση","Σύνδεση με εκχείλωση","Σύνδεση με εκχείλωση"]
["","Συμπυκνωμάτων","","","VP20 (Εσ. διαμ. 20/Εξ.Διάμ. 26), ύψος αποστράγγισης 625 mm","VP20 (Εσ. διαμ. 20/Εξ.Διάμ. 26), ύψος αποστράγγισης 625 mm","VP20 (Εσ. διαμ. 20/Εξ.Διάμ. 26), ύψος αποστράγγισης 625 mm","VP20 (Εσ. διαμ. 20/Εξ.Διάμ. 26), ύψος αποστράγγισης 625 mm"]
["Διαστάσεις","Μονάδα","Πλάτος","mm","550","700","1,000","1,400"]
["","","Βάθος","mm","809","809","809","809"]
["","","Ύψος","mm","250","250","250","250"]
["Περίβλημα","Υλικό","","","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα"]
["Power supply","Φάση","","","1~","1~","1~","1~"]
["","Συχνότητα","","Hz","50/60","50/60","50/60","50/60"]
["","Όνομα","","","VE","VE","VE","VE"]
["","Τάση","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Σημειώσεις","","","","(1) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(1) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(1) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(1) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]
["","","","","(2) - Εύρος τάσης: οι μονάδες είναι κατάλληλες για χρήση σε ηλεκτρικά συστήματα στα οποία η τάση που παρέχεται προς τον ακροδέκτη μονάδας δεν είναι χαμηλότερη ή υψηλότερη από τα αναγραφόμενα όρια τάσης.","(2) - Εύρος τάσης: οι μονάδες είναι κατάλληλες για χρήση σε ηλεκτρικά συστήματα στα οποία η τάση που παρέχεται προς τον ακροδέκτη μονάδας δεν είναι χαμηλότερη ή υψηλότερη από τα αναγραφόμενα όρια τάσης.","(2) - Εύρος τάσης: οι μονάδες είναι κατάλληλες για χρήση σε ηλεκτρικά συστήματα στα οποία η τάση που παρέχεται προς τον ακροδέκτη μονάδας δεν είναι χαμηλότερη ή υψηλότερη από τα αναγραφόμενα όρια τάσης.","(2) - Εύρος τάσης: οι μονάδες είναι κατάλληλες για χρήση σε ηλεκτρικά συστήματα στα οποία η τάση που παρέχεται προς τον ακροδέκτη μονάδας δεν είναι χαμηλότερη ή υψηλότερη από τα αναγραφόμενα όρια τάσης."]
["","","","","(3) - Η μέγιστη επιτρεπόμενη διακύμανση εύρους τάσης μεταξύ φάσεων είναι 2%.","(3) - Η μέγιστη επιτρεπόμενη διακύμανση εύρους τάσης μεταξύ φάσεων είναι 2%.","(3) - Η μέγιστη επιτρεπόμενη διακύμανση εύρους τάσης μεταξύ φάσεων είναι 2%.","(3) - Η μέγιστη επιτρεπόμενη διακύμανση εύρους τάσης μεταξύ φάσεων είναι 2%."]
["","","","","(4) - Το MCA αντιπροσωπεύει το μέγιστο ρεύμα εισόδου.","(4) - Το MCA αντιπροσωπεύει το μέγιστο ρεύμα εισόδου.","(4) - Το MCA αντιπροσωπεύει το μέγιστο ρεύμα εισόδου.","(4) - Το MCA αντιπροσωπεύει το μέγιστο ρεύμα εισόδου."]
["","","","","(5) - Επιλέξτε μέγεθος καλωδίου με βάση την τιμή MCA","(5) - Επιλέξτε μέγεθος καλωδίου με βάση την τιμή MCA","(5) - Επιλέξτε μέγεθος καλωδίου με βάση την τιμή MCA","(5) - Επιλέξτε μέγεθος καλωδίου με βάση την τιμή MCA"]