{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSK08-10AW1"]
[]
[]
[]
[]
["","","","","","EPSK08ARW1","EPSK10ARW1"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","1123","1123"]
["","","","Πλάτος","mm","1330","1330"]
["","","","Βάθος","mm","604","604"]
["Βάρος","Μονάδα","","","kg","178","178"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Θέρμανση","Υψ.","m³/min","75.7","75.7"]
["","","Ψύξη","Υψ.","m³/min","75.7","75.7"]
["Εύρος λειτ.","Ψύξη","","Ελάχ.","°CDB","10","10"]
["","","","Μέγ.","°CDB","43","43"]
["Εύρος λειτουργίας","Ζεστό νερό χρήσης","","Ελάχ.","°CDB","-28","-28"]
["Εύρος λειτ.","Ζεστό νερό χρ.","","Μέγ.","°CDB","40","40"]
["Στάθμη ηχητικής ισχύος","Θέρμανση","","Ονομ.","dBA","45 (1)","47 (1)"]
["","Ψύξη","","Ονομ.","dBA","53 (2)","53.2 (2)"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Ονομ.","dBA","32.4 (1)","32.8 (1)"]
["","Ψύξη","","Ονομ.","dBA","37.2 (2)","37.3 (2)"]
["Ψυκτικό μέσο","Τύπος","","","","R-290","R-290"]
["","GWP","","","","3","3"]
["","Φορτίο","","","tCO2Eq","0.003","0.003"]
["","Φορτίο","","","kg","1","1"]
["Συνδέσεις σωληνώσεων","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","10","10"]
["Τροφοδοσία ισχύος","Όνομα","","","","W1","W1"]
["","Φάση","","","","3~","3~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","400","400"]
["Ρεύμα","Συνιστώμενες ασφάλειες","","","A","16","16"]
["Σημειώσεις","","","","","(1) - Μέτρηση σε LWC 47-55°C, Ta DB/WB 7°C/6°C.","(1) - Μέτρηση σε LWC 47-55°C, Ta DB/WB 7°C/6°C."]
["","","","","","(2) - Μέτρηση σε LWC 12-7°C, Ta 35°C.","(2) - Μέτρηση σε LWC 12-7°C, Ta 35°C."]
["","","","","","(3) - Σωληνώσεις επιτόπιας τοποθέτησης 1 1/4\"","(3) - Σωληνώσεις επιτόπιας τοποθέτησης 1 1/4\""]
["","","","","","(4) - Σωληνώσεις επιτόπιας τοποθέτησης 1 1/2\"","(4) - Σωληνώσεις επιτόπιας τοποθέτησης 1 1/2\""]