{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSX14A"]
[]
[]
[]
[]
["","","","","","EPSX14P30AF","EPSX14P50AF"]
["Περίβλημα","Χρώμα","","","","Χρώμα Traffic white (RAL9016), Μαύρο γραφίτη (RAL9011), Jet black (RAL9005)","Χρώμα Traffic white (RAL9016), Μαύρο γραφίτη (RAL9011), Jet black (RAL9005)"]
["","Υλικό","","","","Πολυπροπυλένιο με αντοχή στις κρούσεις","Πολυπροπυλένιο με αντοχή στις κρούσεις"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","1914","1906"]
["","","","Πλάτος","mm","590","785"]
["","","","Βάθος","mm","671","837"]
["Βάρος","Μονάδα","","","kg","84.0","105"]
["PED","Κατηγορία","","","","Είδος 4.3","Είδος 4.3"]
["Στάθμη ηχητικής ισχύος","Ονομ.","","","dBA","49.0","49.0"]
["Στάθμη ηχητικής πίεσης","Ονομ.","","","dBA","35.0","35.0"]
["Εύρος λειτουργίας","Θέρμανση","Πλευρά νερού","Ελάχ.","°C","0 (3)","0 (3)"]
["","","","Μέγ.","°C","0 (3)","0 (3)"]
["","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","0 (3)","0 (3)"]
["","","Πλευρά νερού","Ελάχ.","°C","0 (3)","0 (3)"]
["","","","Μέγ.","°C","0 (3)","0 (3)"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","230","230"]
["Ηλεκτρικός θερμαντήρας","Τροφοδοσία ισχύος","","Όνομα","","6V / 9W","6V / 9W"]
["","","","Φάση","","1~ / 3~","1~ / 3~"]
["","","","Συχνότητα","Hz","50","50"]
["","","","Τάση","V","230/400","230/400"]
["","Συνιστώμενες ασφάλειες","","","A","0 (4)","0 (4)"]
["Σημειώσεις","","","","","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897"]
["","","","","","(2) - Ελάχιστος απαιτούμενος όγκος, εκτός του όγκου στη μονάδα","(2) - Ελάχιστος απαιτούμενος όγκος, εκτός του όγκου στη μονάδα"]
["","","","","","(3) - Ανατρέξτε στα όρια λειτουργίας στο σχέδιο","(3) - Ανατρέξτε στα όρια λειτουργίας στο σχέδιο"]
["","","","","","(4) - Ανατρέξτε στο διάγραμμα καλωδίωσης και στο εγχειρίδιο εγκατάστασης για την σωστή προτεινόμενη ασφάλεια αναλόγως της παροχής ισχύος και της σύνδεσης δικτύου","(4) - Ανατρέξτε στο διάγραμμα καλωδίωσης και στο εγχειρίδιο εγκατάστασης για την σωστή προτεινόμενη ασφάλεια αναλόγως της παροχής ισχύος και της σύνδεσης δικτύου"]