{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EVH"]
[]
[]
[]
[]
["","","","","","ERGA06EAV3H"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","740"]
["","","","Πλάτος","mm","884"]
["","","","Βάθος","mm","388"]
["Βάρος","Μονάδα","","","kg","58.5"]
["Εύρος λειτ.","Ψύξη","","Ελάχ.","°CDB","10"]
["","","","Μέγ.","°CDB","43"]
["Εύρος λειτουργίας","Ζεστό νερό χρήσης","","Ελάχ.","°CDB","-25"]
["Εύρος λειτ.","Ζεστό νερό χρ.","","Μέγ.","°CDB","35"]
["Στάθμη ηχητικής ισχύος","Θέρμανση","","Ονομ.","dBA","60 (1)"]
["","Ψύξη","","Ονομ.","dBA","62 (1)"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","","Ονομ.","dBA","47 (1)"]
["","Ψύξη","","Ονομ.","dBA","49 (1)"]
["Ψυκτικό μέσο","Τύπος","","","","R-32"]
["","GWP","","","","675.0"]
["","Φορτίο","","","tCO2Eq","1.01"]
["","Φορτίο","","","kg","1.50"]
["Συνδέσεις σωληνώσεων","Υγρό","","ΕΞ.ΔΙΑΜ.","mm","6"]
["","Αέριο","","ΕΞ.ΔΙΑΜ.","mm","15.9"]
["","Συμπυκνωμάτων","","Εξ.Διάμ.","mm","18"]
["","Υψομετρική διαφορά","ΕΣ.-ΕΞ.","Μέγ.","m","30.0"]
["","Θερμομόνωση","","","","Σωληνώσεις υγρού και σωληνώσεις αερίου"]
["Τροφοδοσία ισχύος","Όνομα","","","","V3"]
["","Φάση","","","","1N~"]
["","Συχνότητα","","","Hz","50"]
["","Τάση","","","V","230"]
["Ρεύμα","Συνιστώμενες ασφάλειες","","","A","20"]
["Σημειώσεις","","","","","(1) - Ψύξη Ta 35°C - LWE 18°C (DT = 5°C). Θέρμανση Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]