{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSH-D"]
[]
[]
[]
[]
["","","","","","ETSH16P30DA","ETSH16P50DA"]
["Στάθμη ηχ. πίεσης","Ονομ.","","","dBA","32.8","32.8"]
["Εύρος λειτουργίας","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","10","10"]
["","","Πλευρά νερού","Μέγ.","°C","22","22"]
["","","","Ελάχ.","°C","5","5"]
["","Θέρμανση","Πλευρά νερού","Μέγ.","°C","70","70"]
["","","","Min.","°C","15","15"]
["Στάθμη ηχητικής ισχύος","Ονομ.","","","dBA","45.6","45.6"]
["Διαστάσεις","Μονάδα","","Πλάτος","mm","590","785"]
["","","","Βάθος","mm","615","785"]
["","","","Ύψος","mm","1,891","1,896"]
["Casing","Υλικό","","","","Πολυπροπυλένιο με αντοχή στις κρούσεις","Πολυπροπυλένιο με αντοχή στις κρούσεις"]
["","Colour","","","","Χρώμα Traffic white (RAL9016) / Σκούρο γκρι (RAL7011)","Χρώμα Traffic white (RAL9016) / Σκούρο γκρι (RAL7011)"]
["PED","Category","","","","Είδος 4.3","Είδος 4.3"]
["Βάρος","Μονάδα","","","kg","73","90"]
["Power supply","Φάση","","","","1~","1~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","230","230"]
["Ηλεκτρικός θερμαντήρας","Τροφοδοσία ισχύος","","Συχνότητα","Hz","50","50"]
["","","","Όνομα","","3V / 9W","3V / 9W"]
["","","","Φάση","","1~ / 3~","1~ / 3~"]
["Σημειώσεις","","","","","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]