{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSXB16E"]
[]
[]
[]
[]
["","","","","","ETSXB16P50EF","ETSXB16P30EF"]
["Περίβλημα","Χρώμα","","","","Χρώμα Traffic white (RAL9016) / Χρώμα Traffic black (RAL9017)","Χρώμα Traffic white (RAL9016) / Χρώμα Traffic black (RAL9017)"]
["","Υλικό","","","","Πολυπροπυλένιο με αντοχή στις κρούσεις","Πολυπροπυλένιο με αντοχή στις κρούσεις"]
["Διαστάσεις","Μονάδα","","Ύψος","mm","1,910","1,892"]
["","","","Πλάτος","mm","792","594"]
["","","","Βάθος","mm","816","644"]
["Βάρος","Μονάδα","","","kg","100","76"]
["Sound power level","Ονομ.","","","dBA","45.6","45.6"]
["Στάθμη ηχητικής πίεσης","Ονομ.","","","dBA","32.8","32.8"]
["Εύρος λειτουργίας","Θέρμανση","Πλευρά νερού","Min.","°C","0 (2)","0 (2)"]
["","","","Μέγ.","°C","0 (2)","0 (2)"]
["","Ψύξη","Περιβάλλοντος","Ελάχ.","°CDB","0 (2)","0 (2)"]
["","","Πλευρά νερού","Ελάχ.","°C","0 (2)","0 (2)"]
["","","","Μέγ.","°C","0 (2)","0 (2)"]
["Power supply","Φάση","","","","1~","1~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","230","230"]
["Σημειώσεις","","","","","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897","(1) - Απώλεια θερμότητας σύμφωνα με το ΕΝ12897"]
["","","","","","(2) - Ανατρέξτε στα σχέδια ορίων λειτουργίας","(2) - Ανατρέξτε στα σχέδια ορίων λειτουργίας"]