{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Περίβλημα","Χρώμα","","","","Λευκό","Λευκό"]
["","Υλικό","","","","Ρητίνη","Ρητίνη"]
["Διαστάσεις","Μονάδα","","Διαστάσεις-=-Μονάδα-=-Ύψος-=-χιλ.","mm","290","340"]
["","","","Διαστάσεις-=-Μονάδα-=-Πλάτος-=-χιλ.","mm","1050","1200"]
["","","","Διαστάσεις-=-Μονάδα-=-Βάθος-=-χιλ.","mm","269","262"]
["Βάρος","Μονάδα","","","kg","14","18"]
["Ανεμιστήρας","Ταχύτητα ροής αέρα","Ψύξη","Υψ.","m³/min","16.2","23"]
["","","","Μέτρια","m³/min","13.4","21.1"]
["","","","Χαμηλή","m³/min","12.1","18.7"]
["","","Θέρμανση","Υψ.","m³/min","16.9","23"]
["","","","Μέτρια","m³/min","14.2","20.9"]
["","","","Χαμηλή","m³/min","12.7","18.7"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","","dBA","61","65"]
["","Θέρμανση","","","dBA","61","65"]
["Στάθμη ηχητικής πίεσης","Ψύξη","","Υψ.","dBA","45","49"]
["","","","Μέτρια","dBA","42","45"]
["","","","Χαμηλή","dBA","40","41"]
["","Θέρμανση","","Υψ.","dBA","45","49"]
["","","","Μέτρια","dBA","42","45"]
["","","","Χαμηλή","dBA","40","41"]
["Συνδέσεις σωληνώσεων","Υγρό","","Συνδέσεις σωληνώσεων-=-Υγρό-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","9.52","9.52"]
["","Αέριο","","Συνδέσεις σωληνώσεων-=-Αέριο-=-ΕΞ.ΔΙΑΜ.-=-χιλ.","mm","15.9","15.9"]
["","Αποχέτευση","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Τροφοδοσία ισχύος","Φάση","","","","1~","1~"]
["","Συχνότητα","","","Hz","50","50"]
["","Τάση","","","V","220-240","220-240"]
["Στάνταρτ εξαρτήματα","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Σημειώσεις","","","","","(1) - Οι ονομαστικές αποδόσεις ψύξης βασίζονται στα εξής: εσ. θερμοκρ.: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m"]
["","","","","","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m."]
["Στάνταρτ εξαρτήματα","Screw cover","","","","","3"]