{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9"]
[]
[]
[]
[]
["","","","","FAQ71CVEB9","FAQ100CVEB9"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","Υψ.","dBA","45","49"]
["","","Ονομ.","dBA","42","45"]
["","","Μέτρια","dBA","42","45"]
["","","Χαμηλή","dBA","40","41"]
["","Ψύξη","Μέτρια","dBA","42","45"]
["","","Χαμηλή","dBA","40","41"]
["","","Υψ.","dBA","45","49"]
["","","Ονομ.","dBA","42","45"]
["Απόδοση ψύξης","Συνολική απόδοση","Ονομ.","kW","0.051","0.061"]
["Piping connections","Υγρό","ΕΞ.ΔΙΑΜ.","mm","9.52","9.52"]
["","Αέριο","ΕΞ.ΔΙΑΜ.","mm","15.9","15.9"]
["","Αποχέτευση","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","dBA","61","65"]
["","Θέρμανση","","dBA","61","65"]
["Διαστάσεις","Μονάδα","Πλάτος","mm","1,050","1,200"]
["","","Βάθος","mm","238","240"]
["","","Ύψος","mm","290","340"]
["Περίβλημα","Υλικό","","","Ρητίνη","Ρητίνη"]
["","Colour","","","Fresh white ('κατάλευκο')","Fresh white ('κατάλευκο')"]
["Βάρος","Μονάδα","","kg","13","17"]
["Απόδοση θέρμανσης","Συνολική απόδοση","Ονομ.","kW","0.068","0.061"]
["Power supply","Phase","","","1~","1~"]
["","Συχνότητα","","Hz","50","50"]
["","Τάση","","V","220-240","220-240"]