{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / 3MXM-N"]
[]
[]
[]
[]
["","","","","FBA35A2VEB / FBA35A2VEB / 3MXM68N2V1B"]
["Απόδοση ψύξης","Ονομ.","","kW","6.8"]
["Ψύξη χώρου","SEER","","","5.42"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","440"]
["","Απόδοση","Pdesign","kW","6.80"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A"]
["Θέρμανση χώρου (Μέσο κλίμα)","Απόδοση","Pdesign","kW","3.60"]
["","SCOP/A","","","3.81"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","1,323"]
["Ονομαστική απόδοση","Annual energy consumption","","kWh","1,245"]
["","EER","","","2.73"]
["","COP","","","3.24"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","D"]
["","","Θέρμανση","","C"]
["Απόδοση θέρμανσης","Ονομ.","","kW","8.60"]
["Σημειώσεις","","","","(1) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]