{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / RXM-N"]
[]
[]
[]
[]
["","","","","FBA50A2VEB / RXM50N2V1B","FBA60A2VEB / RXM60N2V1B"]
["Απόδοση ψύξης","Ονομ.","","kW","5.00","5.70"]
["Ψύξη χώρου","Ετήσια κατανάλωση ενέργειας","","kWh/a","","337"]
["","Απόδοση","Pdesign","kW","","5.70"]
["Θέρμανση χώρου (Μέσο κλίμα)","Απόδοση","Pdesign","kW","","4.60"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","","1,607"]
["Ονομαστική απόδοση","Annual energy consumption","","kWh","704","818"]
["","EER","","","3.55","3.48"]
["","COP","","","3.83","3.71"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","A","A"]
["","","Θέρμανση","","A","A"]
["Απόδοση θέρμανσης","Ονομ.","","kW","5.50","7.00"]
["Σημειώσεις","","","","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["","","","","(3) - Οι ονομαστικές αποδόσεις ψύξης βασίζονται στα εξής: εσωτερική θερμοκρασία: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m.","(3) - Οι ονομαστικές αποδόσεις ψύξης βασίζονται στα εξής: εσ. θερμοκρ.: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m"]
["","","","","(4) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m.","(4) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m."]
["Ψύξη χώρου","Κατηγορία ενεργειακής αποδοτικότητας","","","","A+"]
["","SEER","","","","5.91"]
["Θέρμανση χώρου (Μέσο κλίμα)","Κατηγορία ενεργειακής αποδοτικότητας","","","","A+"]
["","SCOP/A","","","","4.01"]