{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":10,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FBA35A2VEB / FBA35A2VEB / RZASG71M2V1B","FBA71A2VEB / RZASG71M2V1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZASG125M7V1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZASG140M7V1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZASG100M7V1B (Archived)","FBA50A2VEB / FBA50A2VEB / RZASG100M7V1B (Archived)"]
["Απόδοση ψύξης","Ονομ.","","kW","6.80 (1)","6.80 (1)"]
["Ψύξη χώρου","SEER","","","5.43","6.19"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","438","385"]
["","Απόδοση","Pdesign","kW","6.80","6.80"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A","A++"]
["Θέρμανση χώρου (Μέσο κλίμα)","Απόδοση","Pdesign","kW","4.50","4.50"]
["","SCOP/A","","","3.82","4.01"]
["","Κατηγορία ενεργειακής αποδοτικότητας","","","A","A+"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","1,649","1,571"]
["Απόδοση θέρμανσης","Ονομ.","","kW","7.50 (2)","7.50 (2)"]
["Σημειώσεις","","","","(1) - Ψύξη: T2: εσωτ. θερμ. 26,6°CDB, 19,4°CWB, εξωτ. θερμ. 48°CDB [Btu/hr/W]","(1) - Ψύξη: T2: εσωτ. θερμ. 26,6°CDB, 19,4°CWB, εξωτ. θερμ. 48°CDB [Btu/hr/W]","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19,0°CWB / εξ. θερμοκρασία 35°CDB, ισοδύναμο μήκος σωληνώσεων: 5m / υψομετρική διαφορά: 0m","(1) - Ψύξη: εσωτερική θερμοκρ. 27°CDB, 19,0°CWB / εξ. θερμοκρασία 35°CDB, ισοδύναμο μήκος σωληνώσεων: 5m / υψομετρική διαφορά: 0m","(1) - Οι ονομαστικές αποδόσεις ψύξης βασίζονται στα εξής: εσ. θερμοκρ.: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m","(1) - Οι ονομαστικές αποδόσεις ψύξης βασίζονται στα εξής: εσ. θερμοκρ.: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m"]
["","","","","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m.","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m.","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m.","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m.","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m.","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m."]
["Εξωτερική μονάδα","","","","","","RZASG125M7V1B","RZASG140M7V1B","RZASG100M7V1B","RZASG100M7V1B"]
["Απόδοση ψύξης","Ονομ.","","kW","","","12.1","13.4","9.50","9.50"]
["Απόδοση θέρμανσης","Ονομ.","","kW","","","13.5","15.5","10.8","10.8"]
["Ψύξη χώρου","Απόδοση","Pdesign","kW","","","12.1","13.4","9.50","9.50"]
["","SEER","","","","","8.59","9.67","5.31","5.38"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","","","845","832","626","618"]
["Θέρμανση χώρου (Μέσο κλίμα)","Απόδοση","Pdesign","kW","","","6.00","7.80","6.00","6.00"]
["","SCOP/A","","","","","5.09","5.62","3.80","3.80"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","","","1650","1943","2211","2211"]
["Ψύξη χώρου","Κατηγορία ενεργειακής αποδοτικότητας","","","","","","","A","A"]
["Θέρμανση χώρου (Μέσο κλίμα)","Κατηγορία ενεργειακής αποδοτικότητας","","","","","","","A","A"]