{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":23,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100BVEB / RZQG100L8Y1B","FCAG125BVEB / RZQG125L8Y1B","FCAG140BVEB / RZQG100L8Y1B","FCAG140BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG60BVEB / FCAG60BVEB / RZQG125L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG100L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG71BVEB / RZQG71L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG100BVEB / RZQG71L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG71L8Y1B","FCAG140BVEB / RZQG140L7Y1B"]
["Απόδοση ψύξης","Ονομ.","","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["Απόδοση θέρμανσης","Ονομ.","","kW","","","","","","","","","","","","","","","7.50","","","","15.50"]
["Ονομαστική απόδοση","EER","","","","","","","","","","","","","","","","3.30","3.39","3.30","3.39","3.30","2.50"]
["","COP","","","","","","","","","","","","","","","","","3.97","","","","3.61"]
["","Ετήσια κατανάλωση ενέργειας","","kWh","","","","","","","","","","","","","","","1,003"]
["","Οδηγία για την Ενεργειακή Σήμανση","Ψύξη","","","","","","","","","","","","","","","","A"]
["","","Θέρμανση","","","","","","","","","","","","","","","","A"]
["Ψύξη χώρου","Κατηγορία ενεργειακής αποδοτικότητας","","","","","","","","","","","","","","","","A","A++","A","A++","A"]
["","Απόδοση","Pdesign","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["","SEER","","","","","","","","","","","","","","","","5.10","6.72","5.10","6.80","5.10","6.44"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","","","","","","","","","","","","","","467","355","467","350","467","1,249"]
["Θέρμανση χώρου (Μέσο κλίμα)","Κατηγορία ενεργειακής αποδοτικότητας","","","","","","","","","","","","","","","","A","A+","A","A+","A"]
["","Απόδοση","Pdesign","kW","","","","","","","","","","","","","","6.00","6.33","6.00","6.33","6.00","11.56"]
["","SCOP/A","","","","","","","","","","","","","","","","3.80","4.20","3.80","4.20","3.80","4.27"]
["","Ετήσια κατανάλωση ενέργειας","","kWh/a","","","","","","","","","","","","","","2,211","2,110","2,211","2,110","2,211","3,795"]
["Σημειώσεις","","","","","","","","","","","","","","","","","(1) - Οι ονομαστικές αποδόσεις ψύξης βασίζονται στα εξής: εσωτερική θερμοκρασία: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m.","(1) - Οι ονομαστικές αποδόσεις ψύξης βασίζονται στα εξής: εσωτερική θερμοκρασία: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m.","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(1) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(1) - Οι ονομαστικές αποδόσεις ψύξης βασίζονται στα εξής: εσωτερική θερμοκρασία: 27°CDB, 19°CWB, εξ. θερμοκρ.: 35°CDB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m."]
["","","","","","","","","","","","","","","","","","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m.","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m.","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(2) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(2) - Οι ονομαστικές αποδόσεις θέρμανσης βασίζονται στα εξής: εσωτερική θερμοκρασία: 20°CDB, εξωτερική θερμοκρασία: 7°CDB, 6°CWB, ισοδύναμες σωληνώσεις ψυκτικού: 5m, υψομετρική διαφορά: 0m."]
["","","","","","","","","","","","","","","","","","(3) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","(3) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας","","","","(3) - Δείτε το ξεχωριστό σχέδιο για το εύρος λειτουργίας"]
["","","","","","","","","","","","","","","","","","(4) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","(4) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά","","","","(4) - Συμβουλευτείτε τα ξεχωριστά σχέδια για τα ηλεκτρολογικά χαρακτηριστικά"]
["Εύρος ενεργειακής αποδοτικότητας","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]