{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":60,"n_cols":8,"rows_kept":60,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-F"]
[]
[]
[]
[]
["","","","","FCAHG100FVEB","FCAHG125FVEB","FCAHG140FVEB","FCAHG71FVEB"]
["Στάθμη ηχητικής πίεσης","Θέρμανση","Υψ.","dBA","44","45","45"]
["","","Μέτρια","dBA","39","40","41"]
["","","Χαμηλή","dBA","33","35","37"]
["","Ψύξη","Μέτρια","dBA","39","40","41"]
["","","Χαμηλή","dBA","33","35","37"]
["","","Υψ.","dBA","44","45","45"]
["Στάνταρτ εξαρτήματα","Εγχειρίδιο εγκατάστασης και χειρισμού","","","Εγχειρίδιο εγκατάστασης και χειρισμού","Εγχειρίδιο εγκατάστασης και χειρισμού","Εγχειρίδιο εγκατάστασης και χειρισμού","Εγχειρίδιο εγκατάστασης και χειρισμού"]
["","Εγχειρίδιο εγκατάστασης","","","Εγχειρίδιο εγκατάστασης","Εγχειρίδιο εγκατάστασης","Εγχειρίδιο εγκατάστασης","Εγχειρίδιο εγκατάστασης"]
["Refrigerant","GWP","","","675","675","675","675"]
["Συνδέσεις σωληνώσεων","Υγρό","ΕΞ.ΔΙΑΜ.","χιλ.","9.52","9.52","9.52","9.52"]
["","Αέριο","ΕΞ.ΔΙΑΜ.","χιλ.","15.9","15.9","15.9"]
["","Συμπυκνωμάτων","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Διακοσμητική μάσκα 4","Διαστάσεις","Βάθος","χιλ.","950","950","950","950"]
["","","Πλάτος","χιλ.","950","950","950","950"]
["","","Ύψος","χιλ.","50","50","50","50"]
["","Μοντέλο","","","BYCQ140D7W1 - λευκό με γκρι γρίλιες","BYCQ140D7W1 - λευκό με γκρι γρίλιες","BYCQ140D7W1 - λευκό με γκρι γρίλιες","BYCQ140D7W1 - λευκό με γκρι γρίλιες"]
["","Χρώμα","","","Κατάλευκο (RAL 9010)","Κατάλευκο (RAL 9010)","Κατάλευκο (RAL 9010)","Κατάλευκο (RAL 9010)"]
["","Βάρος","","kg","5.4","5.4","5.4","5.4"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","dBA","61","61","61"]
["","Θέρμανση","","dBA","61","61","61"]
["Διαστάσεις","Μονάδα","Πλάτος","χιλ.","840","840","840","840"]
["","","Βάθος","χιλ.","840","840","840","840"]
["","","Ύψος","χιλ.","288","288","288","288"]
["Περίβλημα","Υλικό","","","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα","Γαλβανισμένο χαλυβδοέλασμα"]
["Βάρος","Μονάδα","","kg","26.0","26.0","26.0","25.0"]
["Διακοσμητική μάσκα","Βάρος","","kg","10","10","10"]
["","Μοντέλο","","","BYCQ140D7GFW1 - πάνελ αυτοκαθαρισμού με λεπτό φίλτρο με κυψελωτό πλέγμα","BYCQ140D7GFW1 - πάνελ αυτοκαθαρισμού με λεπτό φίλτρο με κυψελωτό πλέγμα","BYCQ140D7GFW1 - πάνελ αυτοκαθαρισμού με λεπτό φίλτρο με κυψελωτό πλέγμα"]
["","Διαστάσεις","Ύψος","χιλ.","130","130","130"]
["","","Βάθος","χιλ.","950","950","950"]
["","","Πλάτος","χιλ.","950","950","950"]
["","Χρώμα","","","Λευκό (RAL 9010)","Λευκό (RAL 9010)","Λευκό (RAL 9010)"]
["Power supply","Φάση","","","1~","1~","1~","1~"]
["","Συχνότητα","","Hz","50/60","50/60","50/60","50/60"]
["","Όνομα","","","VE","VE","VE","VE"]
["","Τάση","","V","220-240","220-240","220-240","220-240"]
["Σημειώσεις","","","","(1) - Οι μονώσεις του BYCQ140D7W1W είναι λευκές. Σας ενημερώνουμε ότι η συσσώρευση ακαθαρσιών στο λευκό είναι πολύ περισσότερο εμφανής και συνεπώς η τοποθέτηση της διακοσμητικής μάσκας του BYCQ140W1W σε περιβάλλοντα που είναι εκτεθειμένα σε συσσωρεύσεις ακαθαρσιών δεν συνιστάται.","(1) - Οι μονώσεις του BYCQ140D7W1W είναι λευκές. Σας ενημερώνουμε ότι η συσσώρευση ακαθαρσιών στο λευκό είναι πολύ περισσότερο εμφανής και συνεπώς η τοποθέτηση της διακοσμητικής μάσκας του BYCQ140W1W σε περιβάλλοντα που είναι εκτεθειμένα σε συσσωρεύσεις ακαθαρσιών δεν συνιστάται.","(1) - Οι μονώσεις του BYCQ140D7W1W είναι λευκές. Σας ενημερώνουμε ότι η συσσώρευση ακαθαρσιών στο λευκό είναι πολύ περισσότερο εμφανής και συνεπώς η τοποθέτηση της διακοσμητικής μάσκας του BYCQ140W1W σε περιβάλλοντα που είναι εκτεθειμένα σε συσσωρεύσεις ακαθαρσιών δεν συνιστάται.","(1) - Οι μονώσεις του BYCQ140D7W1W είναι λευκές. Σας ενημερώνουμε ότι η συσσώρευση ακαθαρσιών στο λευκό είναι πολύ περισσότερο εμφανής και συνεπώς η τοποθέτηση της διακοσμητικής μάσκας του BYCQ140W1W σε περιβάλλοντα που είναι εκτεθειμένα σε συσσωρεύσεις ακαθαρσιών δεν συνιστάται."]
["","","","","(2) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(2) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(2) - Περιέχει φθοριούχα αέρια του θερμοκηπίου","(2) - Περιέχει φθοριούχα αέρια του θερμοκηπίου"]
["","","","","(3) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(3) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(3) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή.","(3) - Η στάθμη ηχητικής ισχύος είναι μία απόλυτη τιμή που αντιστοιχεί στην ισχύ που παράγεται από μία ηχητική πηγή."]
["Στάθμη ηχητικής πίεσης","Θέρμανση","Υψ.","dBA","","","","36"]
["","","Μέτρια","dBA","","","","33"]
["","","Χαμηλή","dBA","","","","29"]
["","Ψύξη","Μέτρια","dBA","","","","33"]
["","","Χαμηλή","dBA","","","","29"]
["","","Υψ.","dBA","","","","36"]
["Συνδέσεις σωληνώσεων","Αέριο","ΕΞ.ΔΙΑΜ.","χιλ.","","","","15.9"]
["","Συμπυκνωμάτων","","","","","","VP25 (I.D. 25/O.D. 32)"]
["Στάθμη ηχητικής ισχύος","Ψύξη","","dBA","","","","53"]
["","Θέρμανση","","dBA","","","","53"]
["Διακοσμητική μάσκα","Βάρος","","kg","","","","10"]
["","Μοντέλο","","","","","","BYCQ140D7GFW1 - πάνελ αυτοκαθαρισμού με λεπτό φίλτρο με κυψελωτό πλέγμα"]
["","Διαστάσεις","Ύψος","χιλ.","","","","130"]
["","","Βάθος","χιλ.","","","","950"]
["","","Πλάτος","χιλ.","","","","950"]
["","Χρώμα","","","","","","Λευκό (RAL 9010)"]